; Copyright (c) Microsoft Corporation.  All rights reserved.

[Version]
Signature="$WINDOWS NT$"
Class=System
ClassGuid={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%MSFT%
PnpLockdown=1
DriverVer = 06/21/2006,10.0.19041.1202

[SourceDisksNames]
3426=windows cd

[SourceDisksFiles]
msisadrv.sys    = 3426
isapnp.sys      = 3426

[DestinationDirs]
DefaultDestDir = 12                ; DIRID_DRIVERS

[ControlFlags]
BasicDriverOk=*
ExcludeFromSelect=*

[Manufacturer]
%GENDEV_MFG%=GENDEV_SYS,NTamd64
%ACC_MFG%=ACC_SYS,NTamd64
%ACER_MFG%=ACER_SYS,NTamd64
%ALI_MFG%=ALI_SYS,NTamd64
%AMD_MFG%=AMD_SYS,NTamd64
%ATI_MFG%=ATI_SYS,NTamd64
%COMPAQ_MFG%=COMPAQ_SYS,NTamd64
%CONTAQ_MFG%=CONTAQ_SYS,NTamd64
%CYRIX_MFG%=CYRIX_SYS,NTamd64
%HITACHI_MFG%=HITACHI_SYS,NTamd64
%HP_MFG%=HP_SYS,NTamd64
%IBM_MFG%=IBM_SYS,NTamd64
%INTEL_MFG%=INTEL_SYS,NTamd64
%MICRON_MFG%=MICRON_SYS,NTamd64
%NATSEMI_MFG%=NATSEMI_SYS,NTamd64
%NEC_MFG%=NEC_SYS,NTamd64
%NVIDIA_MFG%=NVIDIA_SYS,NTamd64
%OPTI_MFG%=OPTI_SYS,NTamd64
%SERVERWORKS_MFG%=SERVERWORKS_SYS,NTamd64
%SIS_MFG%=SIS_SYS,NTamd64
%SMSC_MFG%=SMSC_SYS,NTamd64
%TOSHIBA_MFG%=TOSHIBA_SYS,NTamd64
%UMC_MFG%=UMC_SYS,NTamd64
%VIA_MFG%=VIA_SYS,NTamd64
%VLSI_MFG%=VLSI_SYS,NTamd64
%LEGACY_MFG%=LEGACY_SYS,NTamd64

[GENDEV_SYS.NTamd64]
%PCI\CC_0601_Desc%       = MSISADRV, PCI\CC_0601       ; PCI-ISA BRIDGE
%PCI\CC_0602_Desc%       = MSISADRV, PCI\CC_0602       ; PCI-EISA BRIDGE
%PCI\CC_0600_Desc%       = NO_DRV, PCI\CC_0600         ; HOST PCI BRIDGE
%PCI\CC_0500_Desc%       = NO_DRV,PCI\CC_0500          ; RAM Controller

%*PNP0A00_Desc% = MSISADRV, *PNP0A00       ; ISA BUS
%*PNP0A01_Desc% = MSISADRV, *PNP0A01       ; EISA BUS
%*PNP0A04_Desc% = MSISADRV, *PNP0A04       ; VL BUS
%*PNP0000_Desc% = NO_DRV_PIC, *PNP0000     ; PIC
%*PNP0001_Desc% = NO_DRV_PIC, *PNP0001     ; EISA PIC
%*PNP0003_Desc% = NO_DRV_PIC, *PNP0003     ; APIC
%*PNP0004_Desc% = NO_DRV_PIC, *PNP0004     ; Cyrix SLiC MPIC
%*PNP0100_Desc% = NO_DRV_X, *PNP0100       ; System Timer
%*PNP0101_Desc% = NO_DRV_X, *PNP0101       ; EISA System Timer
%*PNP0103_Desc% = NO_DRV_HPET, *PNP0103    ; HPET
%*PNP0200_Desc% = NO_DRV_X, *PNP0200       ; DMA
%*PNP0201_Desc% = NO_DRV_X, *PNP0201       ; EISA DMA
%*PNP0800_Desc% = NO_DRV_X, *PNP0800       ; System Speaker
%*PNP0B00_Desc% = NO_DRV_X, *PNP0B00       ; Real Time Clock
%*PNP0A05_Desc% = NO_DRV_X_PNP, *PNP0A05   ; Generic ACPI Bus
%*PNP0A06_Desc% = NO_DRV_X_PNP, *PNP0A06   ; Extended IO Bus
%*PNP0C00_Desc% = NO_DRV_X, *PNP0C00       ; PnP BIOS
%*PNP0C01_Desc% = NO_DRV_MBRES, *PNP0C01   ; System board
%*PNP0C02_Desc% = NO_DRV_MBRES, *PNP0C02   ; Motherboard resources
%*PNP0C04_Desc% = NO_DRV_X, *PNP0C04       ; Numeric processor
%*PNP0C09_Desc% = NO_DRV, *PNP0C09         ; Embedded Controller
%*PNP0C0B_Desc% = NO_DRV, *PNP0C0B         ; APM FAN
%*PNP0C0C_Desc% = NO_DRV, *PNP0C0C         ; APM Power Button
%*PNP0C0D_Desc% = NO_DRV, *PNP0C0D         ; APM Lid
%*PNP0C0E_Desc% = NO_DRV, *PNP0C0E         ; APM Sleep Button
%*PNP0C15_Desc% = NO_DRV, *PNP0C15         ; Docking Station
%*PNP0C32_Desc% = NO_DRV, *PNP0C32         ; Direct Application Launch Button
%*PNP0D80_Desc% = NO_DRV_GEN, *PNP0D80     ; Standard Power Management Controller
;%*PNP0C05_Desc% = NO_DRV, *PNP0C05        ; APM BIOS
;%*PNP0C0A_Desc% = NO_DRV, *PNP0C0A        ; APM Battery
;%*PNP0C0F_Desc% = NO_DRV, *PNP0C0F        ; ACPI IRQ Holder
;%*PNP0C13_Desc% = NO_DRV, *PNP0C13        ; PnP BIOS in ACPI fail safe

%ACPI0004_Desc% = NO_DRV_X_PNP, *ACPI0004					; Generic ACPI Bus - Module Device
%ACPI0004_Desc% = NO_DRV_X_PNP, ACPI0004					; Generic ACPI Bus - Module Device
%ACPI0010_Desc% = NO_DRV_X_PNP, *ACPI0010					; Generic ACPI Processor Container Device/
%ACPI\FixedButton_Desc% = NO_DRV, ACPI\FixedButton 				; ACPI Fixed Feature Button
%ACPI\ThermalZone_Desc% = NO_DRV, ACPI\ThermalZone				; ACPI Thermal Zone
%ACPI\DockDevice_Desc% = NO_DRV, ACPI\DockDevice				; ACPI Dock Device
%ACPI\DockDevice_Desc% = MS_TPDOCK, ACPI\DockDevice&_SB_.PCI_.OAK_		; ACPI Dock Device (TP 570 Dock)
%ACPI\DockDevice_Desc% = MS_TPSLICE, ACPI\DockDevice&_SB_.PCI_.ISA_.SLCE	; ACPI Dock Device (TP 570 Slice)

%ISAPNP\ReadDataPort_Desc% = NO_DRV, ISAPNP\ReadDataPort
%*LEGACYISAPNP_Desc% = LEGACY_ISAPNP_DRV, *LEGACYISAPNP				; References LEGACY_ISAPNP_DRV files
%LPTENUM\MicrosoftRawPort958A_Desc% = NO_DRV, LPTENUM\MicrosoftRawPort958A	; Printer Port Logical Interface

[ACC_SYS.NTamd64]
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_10AA&DEV_0000

[ACER_SYS.NTamd64]
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1025&DEV_1435

[ALI_SYS.NTamd64]
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_10B9&DEV_1445
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_10B9&DEV_1449
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_10B9&DEV_1451
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_10B9&DEV_1489
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_10B9&DEV_1521
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_10B9&DEV_1523
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_10B9&DEV_1531
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_10B9&DEV_1533
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_10B9&DEV_1541
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_10B9&DEV_1621
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_10B9&DEV_1647
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_10B9&DEV_1651
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_10B9&DEV_7101

[AMD_SYS.NTamd64]
%IommuDevice_Desc% = NO_DRV,PCI\VEN_1002&DEV_5A23		 		
%ConfigurationDevice_Desc% = NO_DRV,PCI\VEN_1022&DEV_1100              
%ConfigurationDevice_Desc% = NO_DRV,PCI\VEN_1022&DEV_1101              
%ConfigurationDevice_Desc% = NO_DRV,PCI\VEN_1022&DEV_1102              
%ConfigurationDevice_Desc% = NO_DRV,PCI\VEN_1022&DEV_1103              
%IommuDevice_Desc% = NO_DRV,PCI\VEN_1022&DEV_1419                		
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_1022&DEV_740B      
%PowerManagementController_Desc% = NO_DRV,PCI\VEN_1022&DEV_7413       
%PowerManagementController_Desc% = NO_DRV,PCI\VEN_1022&DEV_7443       
%InterruptController_Desc% = NO_DRV,PCI\VEN_1022&DEV_7451              
%InterruptController_Desc% = NO_DRV,PCI\VEN_1022&DEV_7459              
%SmBus_Desc% = NO_DRV,PCI\VEN_1022&DEV_746A         			
%ChipsetController_Desc% = NO_DRV,PCI\VEN_1022&DEV_746B                
%SmBus_Desc% = NO_DRV,PCI\VEN_1022&DEV_780B                		

[ATI_SYS.NTamd64]
%SmBus_Desc% = NO_DRV,PCI\VEN_1002&DEV_4372
%LpcController_Desc% = MSISADRV,PCI\VEN_1002&DEV_4377
%SmBus_Desc% = NO_DRV_MEM,PCI\VEN_1002&DEV_4385
%LpcController_Desc% = MSISADRV,PCI\VEN_1002&DEV_438D

[COMPAQ_SYS.NTamd64]
%PciToEisaBridge_Desc% = MSISADRV, PCI\VEN_0E11&DEV_0001
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_0E11&DEV_0002
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_0E11&DEV_1000
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_0E11&DEV_2000
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_0E11&DEV_AE29
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_0E11&DEV_AE2B
%PciController_Desc% = NO_DRV, PCI\VEN_0E11&DEV_A0F0
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_0E11&DEV_A0F3
%PciController_Desc% = NO_DRV, PCI\VEN_0E11&DEV_A0F7
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_0E11&DEV_AE2A
%PciController_Desc% = NO_DRV, PCI\VEN_0E11&DEV_AE31
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_0E11&DEV_AE69
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_0E11&DEV_AE6C&CC_0600
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_0E11&DEV_AE6D
%PciController_Desc% = NO_DRV, PCI\VEN_8086&DEV_123F&SUBSYS_A2F90E11
%ThermalControlDevice_Desc% = NO_DRV, *CPQA0EF 
%ThermalControlDevice_Desc% = NO_DRV, *CPQAE08
%LegacyDevice_Desc% = NO_DRV, *CPQAE30
%LegacyDevice_Desc% = NO_DRV, *CPQAE3B
%LegacyDevice_Desc% = NO_DRV, *CPQAE3C
%LegacyDevice_Desc% = NO_DRV, *CPQAE4A
%LegacyDevice_Desc% = NO_DRV, *CPQAE4B
%LegacyDevice_Desc% = NO_DRV, *CPQAE4C
%LegacyDevice_Desc% = NO_DRV, *CPQAE4D
%LegacyDevice_Desc% = NO_DRV, *CPQAE53
%LegacyDevice_Desc% = NO_DRV, *CPQAE54
%LegacyDevice_Desc% = NO_DRV, *CPQAE55
%LegacyDevice_Desc% = NO_DRV, *CPQB05F
%LegacyDevice_Desc% = NO_DRV, *CPQB118
%LegacyDevice_Desc% = NO_DRV, *CPQB119
%LegacyDevice_Desc% = NO_DRV, *CPQB11A
%LegacyDevice_Desc% = NO_DRV, *CPQFA1B       

[CONTAQ_SYS.NTamd64]
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1080&DEV_0600

[CYRIX_SYS.NTamd64]
%PciToIsaBridge_Desc% = MSISADRV,PCI\VEN_1078&DEV_0000
%PciToIsaBridge_Desc% = MSISADRV,PCI\VEN_1078&DEV_0002

[HITACHI_SYS.NTamd64]
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1054&DEV_3005
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1054&DEV_3006

[HP_SYS.NTamd64]
%InterruptController_Desc% = NO_DRV, PCI\VEN_103C&DEV_10C1
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_103C&DEV_10ED
%PciController_Desc% = NO_DRV, PCI\VEN_103C&DEV_1219
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_103C&DEV_121A
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_103C&DEV_121B
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_103C&DEV_121C
%LegacyDevice_Desc% = NO_DRV, *HWPC209

[IBM_SYS.NTamd64]
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1014&DEV_000A
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1014&DEV_0017
%ConfigurationDevice_Desc% = NO_DRV, *IBM006A

[INTEL_SYS.NTamd64]
%LegacyDevice_Desc% = NO_DRV_MEM, *INT0800
%SgxDevice_Desc% = NO_DRV_GEN, ACPI\INT0E0C
%ChipsetController_Desc% = NO_DRV, PCI\VEN_8086&DEV_0008
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0040
%ThermalControlDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_0050
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_0051
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0069
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0100
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0104
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0108
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0150
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0154
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0158
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_015C
%InterruptController_Desc% = NO_DRV, PCI\VEN_8086&DEV_0326
%InterruptController_Desc% = NO_DRV, PCI\VEN_8086&DEV_0327
%InterruptController_Desc% = NO_DRV, PCI\VEN_8086&DEV_0331
%InterruptController_Desc% = NO_DRV, PCI\VEN_8086&DEV_0333
%MemoryController_Desc% = NO_DRV, PCI\VEN_8086&DEV_0334
%InterruptController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0371
%InterruptController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0373
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0374
%LegacyDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_0434
%LegacyDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_043E
%PciToEisaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_0482
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_8086&DEV_0483
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_0484
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_0486
%CpuToPciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_04A3&REV_00
%CpuToPciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_04A3&REV_01
%CpuToPciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_04A3&REV_02
%CpuToPciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_04A3&REV_03
%CpuToPciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_04A3
%SpiController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0800
%SpiController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0801
%I2cDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_0802
%I2cDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_0803
%I2cDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_0804
%ChipsetController_Desc% = NO_DRV,PCI\VEN_8086&DEV_080D
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_0813
%SpiController_Desc% = NO_DRV,PCI\VEN_8086&DEV_0815
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_0817
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_1130
%InterruptController_Desc% = NO_DRV_MEM, PCI\VEN_8086&DEV_1161
%CpuToPciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_1225
%CpuToPciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_122D
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_122E
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_1234
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_8086&DEV_1235
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_8086&DEV_1237
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_123C
%InterruptController_Desc% = NO_DRV, PCI\VEN_8086&DEV_123D
%PciController_Desc% = NO_DRV, PCI\VEN_8086&DEV_123F
%CpuToPciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_1250
%InterruptController_Desc% = NO_DRV, PCI\VEN_8086&DEV_1361
%InterruptController_Desc% = NO_DRV, PCI\VEN_8086&DEV_1461
%PciController_Desc% = NO_DRV, PCI\VEN_8086&DEV_1462
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_1A21
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_1A30
%ChipsetController_Desc% = NO_DRV, PCI\VEN_8086&DEV_1A38
%SmBus_Desc% = NO_DRV,PCI\VEN_8086&DEV_1C22
%ThermalControlDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_1C24
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C40
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C41
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C42
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C43
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C44
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C46
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C47
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C49
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C4A
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C4B
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C4C
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C4D
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C4E
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C4F
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C50
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C52
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C54
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C56
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C58
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C59
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C5A
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1C5C
%SmBus_Desc% = NO_DRV,PCI\VEN_8086&DEV_1D22
%ThermalControlDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_1D24
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1D40
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1D41
%SmBus_Desc% = NO_DRV,PCI\VEN_8086&DEV_1D73
%LegacyDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_1D76
%PciController_Desc% = NO_DRV,PCI\VEN_8086&DEV_1D77
%SmBus_Desc% = NO_DRV,PCI\VEN_8086&DEV_1D70
%SmBus_Desc% = NO_DRV,PCI\VEN_8086&DEV_1D71
%SmBus_Desc% = NO_DRV,PCI\VEN_8086&DEV_1D72
%SmBus_Desc% = NO_DRV,PCI\VEN_8086&DEV_1E22
%ThermalControlDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_1E24
%ChipsetController_Desc% = NO_DRV,PCI\VEN_8086&DEV_1E31
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E41
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E42
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E43
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E44
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E46
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E47
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E48
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E49
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E4A
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E53
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E55
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E56
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E57
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E58
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E59
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E5B
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E5D
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E5E
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_1E5F
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_2310
%SmBus_Desc% = NO_DRV,PCI\VEN_8086&DEV_2330
%PerformanceCounter_Desc% = NO_DRV,PCI\VEN_8086&DEV_2331
%ThermalControlDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2332
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2352
%WatchdogTimer_Desc% = NO_DRV,PCI\VEN_8086&DEV_2360
%LegacyDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2364
%LegacyDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2365
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_2410
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_2413
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_2420
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_2423
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_2440
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_2443
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_244C
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2480
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_2483
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_248C
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_24C0
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_24C3
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_24CC
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_24D0
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_24D3
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_24DC
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2500
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2501
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_250B
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2530
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2531
%ChipsetController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2540
%ChipsetController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2541
%ChipsetController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2544
%ChipsetController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2546
%ChipsetController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2548
%ChipsetController_Desc% = NO_DRV, PCI\VEN_8086&DEV_254C
%ChipsetController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2550
%ChipsetController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2551
%PciBridge_Desc% = NO_DRV, PCI\VEN_8086&DEV_2554
%ChipsetController_Desc% = NO_DRV, PCI\VEN_8086&DEV_255D
%PciBridge_Desc% = NO_DRV, PCI\VEN_8086&DEV_2560
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2570
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2576
%MemoryController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2578
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_257E
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2580
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2584
%MemoryController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2588
%CpuToDramController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2590
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_25A1
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_25A4
%WatchdogTimer_Desc% = NO_DRV, PCI\VEN_8086&DEV_25AB
%MemoryController_Desc% = NO_DRV, PCI\VEN_8086&DEV_25AC
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_25C0
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_25D0
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_25D4
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_25D8
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_25F0
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_25F1
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_25F3
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_25F5
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_25F6
%ChipsetController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2600
%LegacyDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_260C
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2610
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2611
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2612
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2613
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2614
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2615
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2617
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2618
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2619
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_261A
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_261B
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_261C
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_261D
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_261E
%LegacyDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2620
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2621
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2622
%ConfigurationDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2623
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2624
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2625
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2626
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2627
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2640
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2641
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2642
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_266A
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2670
%SmBus_Desc% = NO_DRV,PCI\VEN_8086&DEV_269B
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2770
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2774
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2778
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_277C
%CpuToDramController_Desc% = NO_DRV,PCI\VEN_8086&DEV_27A0
%CpuToDramController_Desc% = NO_DRV, PCI\VEN_8086&DEV_27AC
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_27B0
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_27B8
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_27B9
%LpcController_Desc% = MSISADRV,PCI\VEN_8086&DEV_27BC
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_27BD
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_27DA
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2810
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2811
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2812
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2814
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2815
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_283E
%ThermalControlDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_284F
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2910
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2911
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2912
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2914
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2916
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2917
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2918
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_2919
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_2930
%ThermalControlDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_2932
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2970
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_2980
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2990
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_29A0
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_29B0
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_29C0
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_29D0
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_29E0
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_29F0
%CpuToDramController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2A00
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2A09
%CpuToDramController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2A10
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2A19
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2A29
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2A39
%CpuToDramController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2A40
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2A49
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2A59
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2A69
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2A79
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2A89
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2A99
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2AA9
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2AB9
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2AC9
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2AD9
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2AE9
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2AF9
%ConfigurationDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B00
%ConfigurationDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B02
%ConfigurationDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B68
%ConfigurationDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B6A
%PowerManagementController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B04
%CachingAgent_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B08
%CachingAgent_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B0C
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B10
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B14
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B16
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B13
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B18
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B1C
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B1E
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B1B
%CacheCoherenceEngine_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B20
%ConfigurationDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B22
%CacheCoherenceEngine_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B24
%CacheCoherenceEngine_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B28
%ConfigurationDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B2A
%CacheCoherenceEngine_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B2C
%CacheCoherenceEngine_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B30
%CacheCoherenceEngine_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B34
%CacheCoherenceEngine_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B38
%CacheCoherenceEngine_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B3C
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B40
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B42
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B44
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B46
%DebugDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B48
%DebugDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B4C
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B50
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B52
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B54
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B56
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B58
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B5A
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B5C
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B5E
%SmiPort_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B60
%SmiPort_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B62
%SmiPort_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B64
%SmiPort_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B66
%CacheCoherenceEngine_Desc% = NO_DRV,PCI\VEN_8086&DEV_2B6C
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C01
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C10
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C11
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C14
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C15
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C18
%AddressDecoder_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C19
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C1A
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C1C
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C20
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C21
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C22
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C23
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C28
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C29
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C2A
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C2B
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C30
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C31
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C32
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C33
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C40
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C41
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C50
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C51
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C52
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C53
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C54
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C55
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C56
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C57
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C70
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C81
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C90
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C91
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C98
%AddressDecoder_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C99
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C9A
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2C9C
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2CA0
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2CA1
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2CA2
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2CA3
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2CA8
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2CA9
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2CAA
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2CAB
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2D81
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2D90
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2D91
%PhysicalLayerPort_Desc% = NO_DRV,PCI\VEN_8086&DEV_2D92
%PhysicalLayerPort_Desc% = NO_DRV,PCI\VEN_8086&DEV_2D93
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2D94
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_2D95
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2D98
%AddressDecoder_Desc% = NO_DRV,PCI\VEN_8086&DEV_2D99
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2D9A
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_2D9C
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DA0
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DA1
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DA2
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DA3
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DA8
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DA9
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DAA
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DAB
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DB0
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DB1
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DB2
%MemoryControllerChannel_Desc% = NO_DRV,PCI\VEN_8086&DEV_2DB3
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2E00
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2E08
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2E10
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2E18
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2E20
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2E28
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2E30
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2E38
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2E40
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2E48
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2E58
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2E68
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2E78
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2E88
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_2E90
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2E98
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2EA8
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2EB8
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2EC8
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2ED8
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2EE8
%PerformanceCounter_Desc% = NO_DRV, PCI\VEN_8086&DEV_2EF8
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3340
%IoHubToEsiPortBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_3400
%IoHubToEsiPortBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_3401
%IoHubToEsiPortBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_3402
%IoHubToEsiPortBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_3403
%IoHubToEsiPortBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_3404
%IoHubToEsiPortBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_3405
%IoHubToEsiPortBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_3406
%IoHubToEsiPortBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_3407
%PhysicalLayerPort_Desc% = NO_DRV,PCI\VEN_8086&DEV_3418
%PhysicalLayerPort_Desc% = NO_DRV,PCI\VEN_8086&DEV_3419
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3422
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3423
%PerformanceMonitor_Desc% = NO_DRV,PCI\VEN_8086&DEV_3424
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3425
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3426
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3427
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3428
%QuickdataDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_3429
%QuickdataDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_342A
%QuickdataDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_342B
%QuickdataDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_342C
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_342D
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_342E
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_342F
%QuickdataDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_3430
%QuickdataDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_3431
%QuickdataDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_3432
%QuickdataDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_3433
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3438
%InterruptController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3504
%InterruptController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3505
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_3575
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_3578
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3580
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3584
%CpuToIoController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3585
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3590
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3591
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3592
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3593
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3594
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_359B
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_359E
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_35B0
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_35B1
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_35B5
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_35C8
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3600
%QuickdataDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_360B
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_360C
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_360D
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_360E
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_360F
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3610
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3A10
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3A14
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3A16
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3A18
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3A1A
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3A1E
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_3A30
%ThermalControlDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_3A32
%VirtualizationEngineController_Desc% = NO_DRV, PCI\VEN_8086&DEV_3A51
%SmBus_Desc% = NO_DRV, PCI\VEN_8086&DEV_3A60
%ThermalControlDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_3A62
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B00
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B01
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B02
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B03
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B04
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B05
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B06
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B07
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B08
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B09
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B0A
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B0B
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B0C
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B0D
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B0E
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B0F
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B10
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B11
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B12
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B13
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B14
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B15
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B16
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B17
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B18
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B19
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B1A
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B1B
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B1C
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B1D
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B1E
%LpcController_Desc% = MSISADRV, PCI\VEN_8086&DEV_3B1F
%VirtualizationEngineController_Desc% = NO_DRV, PCI\VEN_8086&DEV_3B30
%ThermalControlDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_3B32
%VirtualizationEngineController_Desc% = NO_DRV, PCI\VEN_8086&DEV_3B53
%DmiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C00
%NontransparentBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C0D
%NontransparentBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C0E
%NontransparentBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C0F
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C20
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C21
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C22
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C23
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C24
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C25
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C26
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C27
%ChipsetController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C28
%ChipsetController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C2A
%InterruptController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C2C
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C2E
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C2F
%PerformanceMonitor_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C40
%PerformanceMonitor_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C43
%PerformanceMonitor_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C44
%PerformanceMonitor_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C45
%PerformanceMonitor_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C46
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C71
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C80
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C83
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C84
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C90
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C93
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C94
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CA0
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CA8
%AddressDecoder_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CAA
%AddressDecoder_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CAB
%AddressDecoder_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CAC
%AddressDecoder_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CAD
%AddressDecoder_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CAE
%ThermalControlDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CB0
%ThermalControlDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CB1
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CB2
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CB3
%ThermalControlDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CB4
%ThermalControlDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CB5
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CB6
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CB7
%CpuToDramController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CB8
%PowerManagementController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CC0
%PowerManagementController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CC1
%PowerManagementController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CC2
%PowerManagementController_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CD0
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CE0
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CE3
%PerformanceMonitor_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CE4
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CE6
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CE8
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CE9
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CEA
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CEB
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CEC
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CED
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CEE
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CEF
%AddressDecoder_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CF4
%AddressDecoder_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CF5
%AddressDecoder_Desc% = NO_DRV,PCI\VEN_8086&DEV_3CF6
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C41
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C42
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C86
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_3C96
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_4000
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_4001
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_4003
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_402D
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_402E
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_4030
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_4031
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_4035
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_4036
%PciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_4110
%MemoryController_Desc% = NO_DRV,PCI\VEN_8086&DEV_65C0
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_65F0
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_65F1
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_65F3
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_65F5
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_65F6
%DmaDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_65FF
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_7000
%CpuToPciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_7030
%CpuToPciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_7100
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_7110&CC_0680
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_7110&CC_0601
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_7110&REV_01&CC_0680
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_7110&REV_01&CC_0601
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_8086&DEV_7113&REV_00
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_8086&DEV_7113&REV_01
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_8086&DEV_7113
%SystemGraphicsController_Desc% = NO_DRV, PCI\VEN_8086&DEV_7120
%SystemGraphicsController_Desc% = NO_DRV, PCI\VEN_8086&DEV_7122
%SystemGraphicsController_Desc% = NO_DRV, PCI\VEN_8086&DEV_7124
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_8086&DEV_7180
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_8086&DEV_7190
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_8086&DEV_7192
%CpuToIoController_Desc% = NO_DRV, PCI\VEN_8086&DEV_7194
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_7198
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_8086&DEV_719B
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_8086&DEV_7600
%SmBus_Desc% = NO_DRV,PCI\VEN_8086&DEV_7603
%LegacyDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_8002
%PciBridge_Desc% = NO_DRV, PCI\VEN_8086&DEV_84C4
%MemoryController_Desc% = NO_DRV, PCI\VEN_8086&DEV_84C5
%DmiDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_A000
%DmiDevice_Desc% = NO_DRV, PCI\VEN_8086&DEV_A010
%PciBridge_Desc% = NO_DRV,PCI\VEN_8086&DEV_B555&SUBSYS_B555119F
%DmiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_D130
%DmiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_D131
%DmiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_D132
%DmiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_D133
%DmiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_D134
%DmiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_D135
%DmiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_D136
%DmiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_D137
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_D150
%QpiDevice_Desc% = NO_DRV,PCI\VEN_8086&DEV_D151
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_D155
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_D156
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_D157
%Registers_Desc% = NO_DRV,PCI\VEN_8086&DEV_D158
%PerformanceMonitor_Desc% = NO_DRV,PCI\VEN_8086&DEV_467D

[MICRON_SYS.NTamd64]
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1042&DEV_3000
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1042&DEV_3010

[NATSEMI_SYS.NTamd64]
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1066&DEV_0001
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1066&DEV_8002
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1066&DEV_0002
%LegacyDevice_Desc% = MSISADRV, PCI\VEN_100B&DEV_0011

[NEC_SYS.NTamd64]
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1033&DEV_00A8&CC_0600
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1033&DEV_00A8&CC_0000
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1033&DEV_00A9&CC_0600
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1033&DEV_00AA&CC_0500
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1033&DEV_00AB&SUBSYS_00AB1033
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1033&DEV_00AC&CC_0600
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1033&DEV_00AD&CC_0600
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1033&DEV_00AE&CC_0600
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1033&DEV_00AF
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1033&DEV_00B0
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1033&DEV_00B1&CC_0600

[NVIDIA_SYS.NTamd64]
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_10DE&DEV_005E
%LpcController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_00D3
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_00E4
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_0052
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_0084
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_00D4
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_0264
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_0368
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_03EB
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_0446
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_0542
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_07D8
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_0752
%PciController_Desc% = NO_DRV, PCI\VEN_10DE&DEV_0AA2

[OPTI_SYS.NTamd64]
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1045&DEV_C822
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1045&DEV_C832
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1045&DEV_C557
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1045&DEV_C558
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1045&DEV_C567
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1045&DEV_C568
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1045&DEV_C700
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1045&DEV_C701

[SERVERWORKS_SYS.NTamd64]
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0005&CC_0600
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0007
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0008
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0009&CC_0600
%IoBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0010&CC_0600
%Northbridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0011&CC_0600
%Northbridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0012&CC_0600
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0013
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0014&CC_0600
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0015
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0016&CC_0600
%Northbridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0017&CC_0600
%IoBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0101&CC_0600
%IoBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0110&CC_0600
%Southbridge_Desc% = MSISADRV, PCI\VEN_1166&DEV_0200
%Southbridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0201&CC_0600
%Southbridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0203&CC_0600
%PciBridge_Desc% = NO_DRV, PCI\VEN_1166&DEV_0205&CC_0600
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1166&DEV_0214&CC_1018
%LpcController_Desc% = MSISADRV, PCI\VEN_1166&DEV_0225
%LpcController_Desc% = MSISADRV, PCI\VEN_1166&DEV_0227
%InterruptController_Desc% = NO_DRV, PCI\VEN_1166&DEV_0230
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1166&DEV_0234&CC_0601

[SIS_SYS.NTamd64]
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1039&DEV_0008
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_1039&DEV_0009
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0406
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1039&DEV_0496
%HostBridge_Desc% = NO_DRV, PCI\VEN1039&DEV_0540
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0630
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0635
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0730
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0735
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0755
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0760
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0756
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0761
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0648
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0649
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0655
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0656
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0661
%PciToLpc_Desc% = MSISADRV, PCI\VEN_1039&DEV_0963
%PciToLpc_Desc% = MSISADRV, PCI\VEN_1039&DEV_0964
%PciToLpc_Desc% = MSISADRV, PCI\VEN_1039&DEV_0965
%PciToLpc_Desc% = MSISADRV, PCI\VEN_1039&DEV_0966
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0662
%HostBridge_Desc% = NO_DRV, PCI\VEN_1039&DEV_0741

[SMSC_SYS.NTamd64]
%PciToIsaBridge_Desc% = MSISADRV,PCI\VEN_1055&DEV_9460
%PowerManagementController_Desc% = NO_DRV,PCI\VEN_1055&DEV_9463

[TOSHIBA_SYS.NTamd64]
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1179&DEV_0601
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1179&DEV_0618
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1179&DEV_0602
%ChipsetController_Desc% = NO_DRV,PCI\VEN_1179&DEV_0603
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1179&DEV_0611

[UMC_SYS.NTamd64]
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1060&DEV_8886
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1060&DEV_886A
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1060&DEV_E886
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1060&DEV_8881
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1060&DEV_0891
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1060&DEV_E881
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1060&DEV_E891

[VIA_SYS.NTamd64]
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0204
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0208
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0238
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0258
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0259
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0269
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0282
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0296
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0305
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0308
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0314
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0324
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0327
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0336
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0340
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0351
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0353
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0364
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0391
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0409
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0501
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1106&DEV_0505
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1106&DEV_0576
%CpuToPciAndPciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1107&DEV_0576
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1106&DEV_0586
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1106&DEV_0596
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0597
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0598
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0601
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0605
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_0691
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1106&DEV_0686
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1204
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1208
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1238
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1258
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1259
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1269
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1282
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1296
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1308
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1314
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1324
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1327
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1336
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1340
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1351
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1353
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1364
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_1409
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2204
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2208
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2238
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2258
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2259
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2269
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2282
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2296
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2308
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2314
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2324
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2327
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2336
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2340
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2351
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2353
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2364
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_2409
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_287B&CC_0600
%ChipsetController_Desc% = NO_DRV, PCI\VEN_1106&DEV_287E
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_1106&DEV_3040
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_1106&DEV_3050
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_1106&DEV_3051
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_1106&DEV_3057
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1106&DEV_3074
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3091
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3099
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3101
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1106&DEV_3109
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3112
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3116
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3123
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3128
%PciToIsaBridge_Desc% = MSISADRV,PCI\VEN_1106&DEV_3147
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3148
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3156
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3168
%PciToIsaBridge_Desc% = MSISADRV,PCI\VEN_1106&DEV_3177
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3188
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3189
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3204
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3205
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3208
%PciToIsaBridge_Desc% = MSISADRV,PCI\VEN_1106&DEV_3227
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3238
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_324B&CC_0600
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1106&DEV_324E
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3258
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3259
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3269
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3282
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1106&DEV_3287
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3296
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3314
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3324
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3327
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3336
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1106&DEV_3337
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3340
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3351
%MemoryControllerChannel_Desc% = NO_DRV, PCI\VEN_1106&DEV_3353
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_3364
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_337B&CC_0600
%MemoryControllerChannel_Desc% = NO_DRV, PCI\VEN_1106&DEV_3409
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4204
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4208
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4238
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4258
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4259
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4269
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4282
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4296
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4308
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4314
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4324
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4327
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4336
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4340
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4351
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_1106&DEV_4353
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_4364
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_1106&DEV_4409
%InterruptController_Desc% = NO_DRV_MEM, PCI\VEN_1106&DEV_5208
%InterruptController_Desc% = NO_DRV_MEM, PCI\VEN_1106&DEV_5238
%InterruptController_Desc% = NO_DRV_MEM, PCI\VEN_1106&DEV_5308
%InterruptController_Desc% = NO_DRV, PCI\VEN_1106&DEV_5327
%InterruptController_Desc% = NO_DRV, PCI\VEN_1106&DEV_5336
%InterruptController_Desc% = NO_DRV_MEM, PCI\VEN_1106&DEV_5340
%InterruptController_Desc% = NO_DRV, PCI\VEN_1106&DEV_5351
%InterruptController_Desc% = NO_DRV, PCI\VEN_1106&DEV_5353
%InterruptController_Desc% = NO_DRV_MEM, PCI\VEN_1106&DEV_5364
%InterruptController_Desc% = NO_DRV, PCI\VEN_1106&DEV_5409
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1106&DEV_6327
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1106&DEV_6340
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1106&DEV_6353
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1106&DEV_6364
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1106&DEV_6409
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7204
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7208
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7238
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7258
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7259
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7269
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7282
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7296
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7308
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7314
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7324
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7327
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7336
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7340
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7351
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7353
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7364
%HostBridge_Desc% = NO_DRV, PCI\VEN_1106&DEV_7409
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1106&DEV_8231
%PowerManagementController_Desc% = NO_DRV, PCI\VEN_1106&DEV_8235
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1106&DEV_8324
%LegacyDevice_Desc% = MSISADRV, PCI\VEN_1106&DEV_8409
%InterruptController_Desc% = NO_DRV_MEM,PCI\VEN_1106&DEV_B113
%LegacyDevice_Desc% = MSISADRV, PCI\VEN_1106&DEV_8353
%LegacyDevice_Desc% = NO_DRV, PCI\VEN_1106&DEV_A353

[VLSI_SYS.NTamd64]
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1004&DEV_0005
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1004&DEV_0006
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1004&DEV_0101
%PciToIsaBridge_Desc% = MSISADRV, PCI\VEN_1004&DEV_0103
%CpuToPciBridge_Desc% = NO_DRV, PCI\VEN_1004&DEV_0104

[LEGACY_SYS.NTamd64]
; Legacy install sections still here for Include/Needs by old INFs.
; Moved to msisadrv.inf
%LegacyDevice_Desc% = ISAPNP_DRV
%LegacyDevice_Desc% = ISAPNP_DOCKONLY_DRV
; Moved to pci.inf
%LegacyDevice_Desc% = PCI_DRV_ROOT
%LegacyDevice_Desc% = PCI_DRV
%LegacyDevice_Desc% = PciIoSpaceNotRequired
%LegacyDevice_Desc% = PciSriovSupported
%LegacyDevice_Desc% = PciAcsNotRequired
%LegacyDevice_Desc% = PciASPMOptIn
%LegacyDevice_Desc% = PciASPMOptOut
%LegacyDevice_Desc% = PciD3ColdSupported
%LegacyDevice_Desc% = PciDoNotUseAcs
%LegacyDevice_Desc% = PciEnableAllBridgeInterrupts
%LegacyDevice_Desc% = PciAtomicsOptIn
%LegacyDevice_Desc% = PciExtraSettleTimeRequired
%LegacyDevice_Desc% = PciIgnoreErrorsDuringPLDR
%LegacyDevice_Desc% = PciForceSBR
%LegacyDevice_Desc% = PciBridgeUseNativeWakeInfo

; Generic ISA Bus / PCI-ISA Bridge / PCI-EISA Bridge
[MSISADRV]
CopyFiles=MsIsaDrv_CopyFiles

[MsIsaDrv_CopyFiles]
msisadrv.sys,,,0x100 ;COPYFLG_PROTECTED_WINDOWS_DRIVER_FILE

[MSISADRV.Services]
AddService = msisadrv, %SPSVCINST_ASSOCSERVICE%, msisadrv_ServiceInstallSection

[msisadrv_ServiceInstallSection]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\msisadrv.sys
LoadOrderGroup = "Boot Bus Extender"
AddReg = msisadrv_ServiceInstallSection_AddReg

[msisadrv_ServiceInstallSection_AddReg]
HKR,,Tag,0x00010001,2

; External INFs may include ISAPNP_DRV section.  This section is provided for
; backwards compatibility with those infs.  New infs should use include
; msisadrv section instead.
[ISAPNP_DRV]
CopyFiles=MsIsaDrv_CopyFiles

[ISAPNP_DRV.Services]
AddService = msisadrv, %SPSVCINST_ASSOCSERVICE%, msisadrv_ServiceInstallSection

; ISA PnP Bus
; The LEGACY_ISAPNP_DRV should only be used for systems which require
; the ability to enumerate devices via ISAPNP protocol.  Most systems should use
; msisadrv.
[LEGACY_ISAPNP_DRV]
CopyFiles=IsaPnp_CopyFiles

[IsaPnp_CopyFiles]
isapnp.sys,,,0x100 ;COPYFLG_PROTECTED_WINDOWS_DRIVER_FILE

[LEGACY_ISAPNP_DRV.Services]
AddService = isapnp, %SPSVCINST_ASSOCSERVICE%, isapnp_ServiceInstallSection, isapnp_EventLogInstallSection

[isapnp_ServiceInstallSection]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\isapnp.sys
LoadOrderGroup = "Boot Bus Extender"
AddReg         = ISAPNP_DRV.AddReg

[ISAPNP_DRV.AddReg]
HKR,,HasBootConfig,0x00010001,00000000

[isapnp_EventLogInstallSection]
AddReg = isapnp_EventLog_AddReg

[isapnp_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\isapnp.sys"
HKR,,TypesSupported,%REG_DWORD%,7

; Dock only PCI-(E)ISA Bridge
; Only neccessary if bridge is located prior to ISA bridge in laptop device
; number-wise
[ISAPNP_DOCKONLY_DRV]
CopyFiles=IsaPnp_CopyFiles

[ISAPNP_DOCKONLY_DRV.HW]
AddReg = ISAPNP_DOCKONLY_DRV_AddReg

[ISAPNP_DOCKONLY_DRV.Services]
AddService = isapnp, %SPSVCINST_ASSOCSERVICE%, isapnp_ServiceInstallSection, isapnp_EventLogInstallSection

[ISAPNP_DOCKONLY_DRV_AddReg]
HKR,,DeferBridge,0x00010001,00000001

; Do-nothing section used to avoid "Unknown hardware" installation prompts.
[NO_DRV]

[NO_DRV.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

; NO_DRV Variation with MUTEing
[NO_DRV_X]
AddReg = NO_DRV_X_REG

[NO_DRV_X.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_X_REG]
HKR,,ResourcePickerExceptions,0,"IO@0-0xFF:*;IO:HAL,MBRES;IRQ:HAL,*"
HKR,,ResourcePickerTags,0,"MBRES"

; NO_DRV Variation with MUTEing
[NO_DRV_X_PNP]
AddReg = NO_DRV_X_PNP_REG

[NO_DRV_X_PNP.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_X_PNP_REG]
HKR,,ResourcePickerExceptions,0,"IO@0-0xFF:*;IO:HAL,MBRES;IRQ:HAL,*"
HKR,,ResourcePickerTags,0,"MBRES"

; NO_DRV Variation - MUTEing for PIC/APIC
[NO_DRV_PIC]
AddReg = NO_DRV_PIC_REG

[NO_DRV_PIC.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_PIC_REG]
HKR,,ResourcePickerExceptions,0,"IO@0-0xFF:*;IO:HAL,MBRES;MEM:HAL,MBRES,*;IRQ:HAL,MBRES,*"
HKR,,ResourcePickerTags,0,"MBRES"

; NO_DRV Variation - MUTEing for HPET
[NO_DRV_HPET]
AddReg = NO_DRV_HPET_REG

[NO_DRV_HPET.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_HPET_REG]
HKR,,ResourcePickerExceptions,0,"MEM:HAL,MBRES,*;IRQ:HAL,MBRES,*"
HKR,,ResourcePickerTags,0,"MBRES"

; NO_DRV Variation - MUTEing/TAGing for motherboard resource
[NO_DRV_MBRES]
AddReg = NO_DRV_MBRES_REG

[NO_DRV_MBRES.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_MBRES_REG]
HKR,,ResourcePickerExceptions,0,"IO:HAL,MBRES,*;MEM:HAL,MBRES,*"
HKR,,ResourcePickerTags,0,"MBRES"

; NO_DRV Variation - MUTEing for MEM only conflicts
[NO_DRV_MEM]
AddReg = NO_DRV_MEM_REG

[NO_DRV_MEM.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[NO_DRV_MEM_REG]
HKR,,ResourcePickerExceptions,0,"MEM:HAL,MBRES,*"
HKR,,ResourcePickerTags,0,"MBRES"

; NO_DRV Variation - Add generic driver installed property
[NO_DRV_GEN]
AddProperty=NO_DRV_GEN_Properties

[NO_DRV_GEN_Properties]
GenericDriverInstalled,,,,1

[NO_DRV_GEN.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

; Overrides for dock eject priority (3rd party INFs should use the ID of the
; _DCK device, ie the one with a OEM hardware ID and a compat ID of PNP0C15)
[MS_TPDOCK]

[MS_TPDOCK.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[MS_TPDOCK.HW]
AddReg = MS_TPDOCK_HW.AddReg

[MS_TPDOCK_HW.AddReg]
HKR,,EjectPriority,0x00010001,00000100

[MS_TPSLICE]

[MS_TPSLICE.Services]
AddService = , %SPSVCINST_ASSOCSERVICE%   ; null service install

[MS_TPSLICE.HW]
AddReg = MS_TPSLICE_HW.AddReg

[MS_TPSLICE_HW.AddReg]
HKR,,EjectPriority,0x00010001,00000080

; Section to provide backwards compatibilty for INFs that are dependent on
; PCI specific machine.inf sections, which were moved to pci.inf

[PCI_DRV_ROOT]
Include=pci.inf
Needs=PCI_ROOT

[PCI_DRV_ROOT.Services]
Include=pci.inf
Needs=PCI_ROOT.Services

[PCI_DRV_ROOT.HW]
Include=pci.inf
Needs=PCI_ROOT.HW

[PCI_DRV]
Include=pci.inf
Needs=PCI_BRIDGE

[PCI_DRV.Services]
Include=pci.inf
Needs=PCI_BRIDGE.Services

[PCI_DRV.HW]
Include=pci.inf
Needs=PCI_BRIDGE.HW

; Section for device INFs to include in their DDInstall section, for features
; that are not detectable by just looking at the device hardware.
;
; Note that these sections provide backwards compatibilty for INFs that are
; dependent on PCI specific machine.inf sections, which were moved to pci.inf.
; New device INFs should include these sections from pci.inf instead.
;
; Example INF usage for PCI-based device:
;
; [PciDevice_Install]
; ...
;
; [PciDevice_Install.HW]
; Include = pci.inf
; Needs   = PciIoSpaceNotRequired.HW, PciSriovSupported.HW
; ...
;
; See pci.inf for all supported feature sections.

; IO space not required.
[PciIoSpaceNotRequired]
Needs=PciIoSpaceNotRequired.HW

[PciIoSpaceNotRequired.HW]
Include=pci.inf
Needs=PciIoSpaceNotRequired.HW

; SRIOV supported.
[PciSriovSupported]
Needs=PciSriovSupported.HW

[PciSriovSupported.HW]
Include=pci.inf
Needs=PciSriovSupported.HW

; ACS not required.
[PciAcsNotRequired]
Needs=PciAcsNotRequired.HW

[PciAcsNotRequired.HW]
Include=pci.inf
Needs=PciAcsNotRequired.HW

; Opt-in to ASPM.
[PciASPMOptIn]
Needs=PciASPMOptIn.HW

[PciASPMOptIn.HW]
Include=pci.inf
Needs=PciASPMOptIn.HW

; Opt-out of ASPM.
[PciASPMOptOut]
Needs=PciASPMOptOut.HW

[PciASPMOptOut.HW]
Include=pci.inf
Needs=PciASPMOptOut.HW

; D3 cold supported.
[PciD3ColdSupported]
Needs=PciD3ColdSupported.HW

[PciD3ColdSupported.HW]
Include=pci.inf
Needs=PciD3ColdSupported.HW

; Prevents Windows from enabling ACS on the Bridge.  Will also prevent
; any feature that requires ACS.
[PciDoNotUseAcs]
Needs=PciDoNotUseAcs.HW

[PciDoNotUseAcs.HW]
Include=pci.inf
Needs=PciDoNotUseAcs.HW

; Normally Windows will filter out bridge interrupts that it does not use.
; Set this flag to disable bridge interrupt filtering.
[PciEnableAllBridgeInterrupts]
Needs=PciEnableAllBridgeInterrupts.HW

[PciEnableAllBridgeInterrupts.HW]
Include=pci.inf
Needs=PciEnableAllBridgeInterrupts.HW

; Opt-in to Atomics.
[PciAtomicsOptIn]
Needs=PciAtomicsOptIn.HW

[PciAtomicsOptIn.HW]
Include=pci.inf
Needs=PciAtomicsOptIn.HW

; Set this flag if a device requires extra
; settle time after D3Cold transitions.
[PciExtraSettleTimeRequired]
Needs=PciExtraSettleTimeRequired.HW

[PciExtraSettleTimeRequired.HW]
Include=pci.inf
Needs=PciExtraSettleTimeRequired.HW

; Set this flag if a device generates
; errors that should be ignored during
; PLDR.
[PciIgnoreErrorsDuringPLDR]
Needs=PciIgnoreErrorsDuringPLDR.HW

[PciIgnoreErrorsDuringPLDR.HW]
Include=pci.inf
Needs=PciIgnoreErrorsDuringPLDR.HW

; Set this flag if a device wants to force Secondary Bus Reset event if
; it has sibling functions.
[PciForceSBR]
Needs=PciForceSBR.HW

[PciForceSBR.HW]
AddReg=PciForceSBR.RegHW

[PciForceSBR.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7, ForceSBR,0x10001,1

; Set this flag if a non-root-integrated bridge wants to determine its lowest
; wake-able D-state in S0 from native PCI PMCSR register
[PciBridgeUseNativeWakeInfo]
Needs=PciBridgeUseNativeWakeInfo.HW

[PciBridgeUseNativeWakeInfo.HW]
AddReg=PciBridgeUseNativeWakeInfo.RegHW

[PciBridgeUseNativeWakeInfo.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7, BridgeUseNativeWakeInfo,0x10001,1

[Strings]

; localizable
MSFT = "Microsoft"
ACC_MFG = "ACC"
ACER_MFG="ACER"
ALI_MFG="ALi"
AMD_MFG = "AMD"
ATI_MFG = "ATI"
COMPAQ_MFG="Compaq"
CONTAQ_MFG = "CONTAQ"
CYRIX_MFG = "CYRIX"
HITACHI_MFG = "Hitachi"
HP_MFG = "Hewlett-Packard"
IBM_MFG = "IBM"
INTEL_MFG = "Intel"
MICRON_MFG = "Micron Electronics"
NATSEMI_MFG = "National Semiconductor"
NEC_MFG = "NEC"
NVIDIA_MFG = "NVIDIA"
OPTI_MFG = "Opti"
SERVERWORKS_MFG = "ServerWorks (RCC)"
SIS_MFG = "Silicon Integrated Systems"
SMSC_MFG = "Standard Microsystems Corp."
TOSHIBA_MFG = "Toshiba"
ULI_MFG = "ULI"
UMC_MFG = "UMC"
VIA_MFG = "VIA"
VLSI_MFG = "VLSI"
LEGACY_MFG = "LEGACY"
GENDEV_MFG = "(Standard system devices)"

; class codes
PCI\CC_0601_Desc = "PCI standard ISA bridge"
PCI\CC_0602_Desc = "PCI standard EISA bridge"
PCI\CC_0500_Desc = "PCI standard RAM Controller"
PCI\CC_0600_Desc = "PCI standard host CPU bridge"

; pnp
*PNP0A00_Desc = "ISA Plug and Play bus"
*PNP0A01_Desc = "EISA bus"
*PNP0A04_Desc = "ISA Plug and Play bus with VL slots"
*PNP0000_Desc = "Programmable interrupt controller"
*PNP0001_Desc = "EISA programmable interrupt controller"
*PNP0003_Desc = "Advanced programmable interrupt controller"
*PNP0004_Desc = "Cyrix SLiC MP interrupt controller"
*PNP0100_Desc = "System timer"
*PNP0101_Desc = "EISA system timer"
*PNP0103_Desc = "High precision event timer"
*PNP0200_Desc = "Direct memory access controller"
*PNP0201_Desc = "EISA direct memory access controller"
*PNP0800_Desc = "System speaker"
*PNP0A05_Desc = "Generic Bus"
*PNP0A06_Desc = "Extended IO Bus"
*PNP0B00_Desc = "System CMOS/real time clock"
*PNP0C00_Desc = "Plug and Play BIOS"
*PNP0C01_Desc = "System board"
*PNP0C02_Desc = "Motherboard resources"
*PNP0C04_Desc = "Numeric data processor"
*PNP0C09_Desc = "Microsoft ACPI-Compliant Embedded Controller"
*PNP0C0B_Desc = "ACPI Fan"
*PNP0C0C_Desc = "ACPI Power Button"
*PNP0C0D_Desc = "ACPI Lid"
*PNP0C0E_Desc = "ACPI Sleep Button"
*PNP0C15_Desc = "Docking Station"
*PNP0C32_Desc = "Direct Application Launch Button"
*PNP0D80_Desc = "Standard Power Management Controller"
;*PNP0C05_Desc = "Advanced Power Management support"
;*PNP0C0A_Desc = "ACPI Battery"
;*PNP0C0F_Desc = "ACPI IRQ Holder for PCI IRQ Steering"
;*PNP0C13_Desc = "Plug and Play BIOS (fail safe)"

; acpi
ACPI0004_Desc = "ACPI Module Device"
ACPI0010_Desc = "ACPI Processor Container Device"
ACPI\FixedButton_Desc = "ACPI Fixed Feature Button"
ACPI\ThermalZone_Desc = "ACPI Thermal Zone"
ACPI\DockDevice_Desc = "Docking Station"
*LEGACYISAPNP_Desc = "Legacy ISAPNP device"
ISAPNP\ReadDataPort_Desc = "ISAPNP Read Data Port"
LPTENUM\MicrosoftRawPort958A_Desc = "Printer Port Logical Interface"

; generic
LegacyDevice_Desc = "Legacy device"
ChipsetController_Desc = "Chipset Controller"
MemoryController_Desc = "Memory Controller"
SmBus_Desc = "SM Bus Controller"
DmaDevice_Desc = "DMA Device"
CpuToPciAndPciToIsaBridge_Desc = "CPU-to-PCI and PCI-to-ISA Bridge"
PciBridge_Desc = "PCI Bridge"
CpuToPciBridge_Desc = "CPU to PCI Bridge"
PciToIsaBridge_Desc = "PCI to ISA Bridge"
PciToEisaBridge_Desc = "PCI to EISA Bridge"
PciToLpc_Desc = "PCI to LPC Bridge"
LpcController_Desc = "LPC Controller"
PowerManagementController_Desc = "Power Management Controller"
IommuDevice_Desc = "IOMMU Device"
PciController_Desc = "PCI Controller"
PerformanceCounter_Desc = "Performance Counter"
PerformanceMonitor_Desc = "Performance Monitor"
Registers_Desc = "Registers"
HostBridge_Desc = "Host Bridge"
InterruptController_Desc = "Interrupt Controller"
CpuToIoController_Desc = "CPU to IO Controller"
ChipsetHostController_Desc = "Chipset Host Controller"
CpuToDramController_Desc = "CPU to DRAM Controller"
WatchdogTimer_Desc = "Watchdog Timer"
ThermalControlDevice_Desc = "Thermal Control Device"
CacheCoherenceEngine_Desc = "Cache Coherence Engine"
CachingAgent_Desc = "Caching Agent"
DebugDevice_Desc = "Debug Device"
QpiDevice_Desc = "QPI Device"
SmiPort_Desc = "SMI Port"
IoHubToEsiPortBridge_Desc = "IO Hub to ESI Port Bridge"
QuickdataDevice_Desc = "QuickData Device"
AddressDecoder_Desc = "Address Decoder"
MemoryControllerChannel_Desc = "Memory Controller Channel"
PhysicalLayerPort_Desc = "Physical Layer Port"
VirtualizationEngineController_Desc = "Virtualization Engine Controller"
NontransparentBridge_Desc = "Non-Transparent Bridge"
SystemGraphicsController_Desc = "System Graphics Controller"
DmiDevice_Desc = "DMI Device"
IoBridge_Desc = "IO Bridge"
Southbridge_Desc = "Southbridge"
Northbridge_Desc = "Northbridge"
I2cDevice_Desc = "I2C Device"
SpiController_Desc = "SPI Controller"
ConfigurationDevice_Desc = "Configuration Device"
SgxDevice_Desc = "SGX Device"

; non-localizable
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_DEMAND_START   = 3
SERVICE_ERROR_NORMAL   = 1
SERVICE_ERROR_CRITICAL = 3
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
