; ** COPYRIGHT (C) 2007-2019 Realtek CORPORATION
;
; Realtek PCIe FE Family Controller
; Realtek PCI GbE Family Controller
; Realtek PCIe GbE Family Controller
; Realtek PCIe 2.5GbE Family Controller
;
; This product is covered by one or more of the following patents:
; US6,570,884, US6,115,776, and US6,327,625.
;

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %MSFT%
DriverVer   = 04/10/2015,9.001.0410.2015

[Manufacturer]
%Realtek%=Realtek, NTamd64

[ControlFlags]
ExcludeFromSelect     = *


[Realtek.NTamd64]
; 8169 Cardbus Jumbo 7k
; remember to remove from OEM INF list
%RTL8169.DeviceDesc% = R8169C7k.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_03351154
; 8169 S-32
%SMC9452TX.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_EE221113


; 8169
%RTL8169.DeviceDesc%        = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&REV_10
%DLINKDGE528T.DeviceDesc%   = RTL8169.ndi, PCI\VEN_1186&DEV_4300&SUBSYS_43001186
%DLINKDGE660TD.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_43011186
%SITECOM.DeviceDesc%        = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_0030182D
%ZYXELGN680T.DeviceDesc%    = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_330B187E
%IODATAETGPCI.DeviceDesc%   = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_D01F10FC
%IODATAETGCB.DeviceDesc%    = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&SUBSYS_D03E10FC


; 8168
%RTL8168.DeviceDesc% = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&REV_01

; 8112
%RTL8168.DeviceDesc% = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83851043&REV_01


; 8101
%RTL8136.DeviceDesc% = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&REV_01

; 8131
%RTL8136.DeviceDesc% = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83A01043&REV_01

; 8101HP
%RTL8136.DeviceDesc% = RTL8136HP.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A89103C ;HP
%RTL8136.DeviceDesc% = RTL8136HP.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_30CB103C ;HP
%RTL8136.DeviceDesc% = RTL8136HP.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;Toshiba

; 8136HP S5 WOL Default Disable
%RTL8136.DeviceDesc% = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A60103C ;HP
%RTL8136.DeviceDesc% = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A79103C ;HP-CPC
%RTL8136.DeviceDesc% = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136.DeviceDesc% = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A59103C ;HP
%RTL8136.DeviceDesc% = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A78103C ;HP-CPC
%RTL8136.DeviceDesc% = RTL8136HPS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A7B103C ;HP


; 8167
%RTL8169.DeviceDesc% = RTL8169.ndi, PCI\VEN_10EC&DEV_8167


; 8168C
%RTL8168.DeviceDesc% = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&REV_02

; 8168C S5 WOL Default Disable
%RTL8168.DeviceDesc% = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A6F103C&REV_02;HP cPC
%RTL8168.DeviceDesc% = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A74103C;HP
%RTL8168.DeviceDesc% = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A7F103C;HP
%RTL8168.DeviceDesc% = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A82103C;HP
%RTL8168.DeviceDesc% = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A85103C;HP
%RTL8168.DeviceDesc% = RTL8168CS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A8A103C;HP

; 8168C_NotSpdDown
%RTL8168.DeviceDesc% = RTL8168CNotSpdDown.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02

; 8168C_Force_Gigabit
%RTL8168.DeviceDesc% = RTL8168CForceGigabit.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83AB1043&REV_02

; 8168CP_Force_100_Full
%RTL8136.DeviceDesc% = RTL8168CForce100Full.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2100146C&REV_02


; 8102E
%RTL8136.DeviceDesc% = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&REV_02

; 8102E S5 WOL Default Disable
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A85103C ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A8A103C ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A8C103C ;HP_eton
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A97103C ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A98103C ;HP_elvas
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A9D103C ;HP_evans
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2A9F103C ;HP_fiano
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AA3103C ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AA4103C ;HP_edwards
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB0103C ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB8103C ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB9103C ;HP

; 8102E S5 WOL Hide and Default Enable
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1414103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1425103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1426103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1427103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1428103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1429103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_142A103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1430103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1431103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1439103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_143A103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_143B103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_143C103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_143F103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1440103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1441103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1442103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1443103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1444103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1445103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1446103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1447103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1448103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1449103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_144A103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_144B103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_144C103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_144D103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1469103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_146A103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_146B103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_146C103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1474103C&REV_02 ;HP_Valima
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1475103C&REV_02 ;HP_Valima
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1476103C&REV_02 ;HP_Villemont
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_147B103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_147C103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1484103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1485103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_148B103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_149C103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_149D103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_149E103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1526103C&REV_02 ;HP_Villemont
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1580103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1581103C&REV_02 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1582103C&REV_02 ;HP

;;Compal 8103EL Force Enable Clock Request
%RTL8136.DeviceDesc% = RTL8102ForceEnableClkReq.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF001179&REV_02 ;TOSHIBA


; 8168D
%RTL8168.DeviceDesc% = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&REV_03

; 8168D S5 WOL Default Disable
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A8E103C ;HP_jesse
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A90103C ;HP_indio
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A92103C ;HP_aloe
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A94103C ;HP_eureka3
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A97103C ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A9C103C ;HP_iona
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA2103C ;HP_boma
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA3103C ;HP_boma-d
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA0103C ;HP_e46
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2A9A103C ;HP_e66
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA5103C ;HP_elkhart
%RTL8168.DeviceDesc% = RTL8168DS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA6103C ;HP_Matadi

; 8168D S5 WOL Hide and Default Enable
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1405103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1407103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1409103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1411103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1412103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1413103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1420103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1421103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1423103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1425103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1426103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1427103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1428103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1429103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142A103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142B103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142C103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_142D103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1430103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1431103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1433103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1434103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1435103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1436103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1437103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_143D103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_143F103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1440103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1441103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1442103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1443103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1448103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1449103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144A103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144B103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144C103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144D103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_144E103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1469103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_146A103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_146B103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_146C103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1474103C&REV_03 ;HP_Valima
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1475103C&REV_03 ;HP_Valima
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1476103C&REV_03 ;HP_Villemont
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_147B103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_147C103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_147F103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1482103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1484103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1485103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1486103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1488103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_148B103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_149B103C&REV_03 ;HP_Fossil2.0
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_149C103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1526103C&REV_03 ;HP_Villemont
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1580103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1581103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1582103C&REV_03 ;HP
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1583103C&REV_03 ;HP_Neon1.0
%RTL8168.DeviceDesc% = RTL8168DS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1590103C&REV_03 ;HP

; 8112L
%RTL8168.DeviceDesc% = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83A31043&REV_03


; 8168DP
%RTL8168.DeviceDesc% = RTL8168DP.ndi, PCI\VEN_10EC&DEV_8168&REV_04


; 8168E
%RTL8168.DeviceDesc% = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&REV_06
%TPLINKPCIEGBE.DeviceDesc% = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_34687470&REV_06 ;TP-Link

; 8168E S5 WOL Default Disable
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17A0103C ;HP_Popeye
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17A1103C ;HP_Magellan
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17A2103C ;HP_Drake
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA7103C ;HP_F01
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AA8103C ;HP_ArnicaF02
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AAB103C ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AAC103C ;HP_Aronia
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AAD103C ;HP_Anhui
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AAE103C ;HP_Alberta
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AB5103C ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AB6103C ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ABB103C ;HP_Inglewood
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ABE103C ;HP_Hudson
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ABF103C ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AC2103C ;HP_Carmel
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AC3103C ;HP_Lavaca
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AC4103C ;HP_Angelino
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AC5103C ;HP_Leon
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AC6103C ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AC8103C ;HP_Angelica
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ACB103C ;HP_Angelino2
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ACD103C ;HP_Hibiscus
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ACE103C ;HP_Pittsburgh
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ACF103C ;HP_Holly
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AD2103C ;HP_PauBrazil2
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AD7103C ;HP_Leon2
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ADC103C ;HP_Lavaca2
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ADD103C ;HP_Inglewood
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AE6103C ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20121854&REV_06 ;LG
%RTL8168.DeviceDesc% = RTL8168ES5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_20131854&REV_06 ;LG

; 8168E S5 WOL Hide and Default Enable
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1592103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1593103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1594103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1595103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1596103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1597103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1599103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_159A103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_159B103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1633103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1634103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1635103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_164F103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1676103C&REV_06 ;HP_Metallica
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1677103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1678103C&REV_06 ;HP_Madonna
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_167C103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_167D103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_167E103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_167F103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1680103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_168B103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_168C103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_168E103C&REV_06 ;HP
%RTL8168.DeviceDesc% = RTL8168ES5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_168F103C&REV_06 ;HP

; 8168E EEE Default Enable
%RTL8168.DeviceDesc% = RTL8168EEEEEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_15B110CF&REV_06 ;Fuji
%RTL8168.DeviceDesc% = RTL8168EEEEEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_16AF10CF&REV_06 ;Fuji

; 8168E EEE Default Enable & S5 WOL Hide and Default Disable
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_907B104D&REV_06 ;SONY
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_907E104D&REV_06 ;SONY
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9083104D&REV_06 ;SONY
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9084104D&REV_06 ;SONY
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9085104D&REV_06 ;SONY
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9086104D&REV_06 ;SONY
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9087104D&REV_06 ;SONY
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9088104D&REV_06 ;SONY
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9089104D&REV_06 ;SONY
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_908B104D&REV_06 ;SONY
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_908D104D&REV_06 ;SONY
%RTL8168.DeviceDesc% = RTL8168EEEEEnS5WOLHideDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_908E104D&REV_06 ;SONY

; 8168E Flow control Default Disable
%RTL8168.DeviceDesc% = RTL8168EEEEDnFCDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_602617AA&REV_06 ;NEC

; 8168ES
%RTL8168.DeviceDesc% = RTL8168ES.ndi, PCI\VEN_10EC&DEV_8168&REV_08


; 8104
%RTL8136.DeviceDesc% = RTL8104.ndi, PCI\VEN_10EC&DEV_8137&REV_03


; 8401
%RTL8136.DeviceDesc% = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&REV_04

; 8401 S5 WOL Hide and Default Enable
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1404103C&REV_04 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1406103C&REV_04 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_140A103C&REV_04 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1415103C&REV_04 ;HP
%RTL8136.DeviceDesc% = RTL8102S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_148A103C&REV_04 ;HP


; 8105E
%RTL8136.DeviceDesc% = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&REV_05

; 8105E S5 WOL Default Disable
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AA7103C ;HP
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AA8103C ;HP
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AA9103C ;HP_Alpinia
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AAD103C ;HP_Anhui
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AAE103C ;HP_Alberta
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AAF103C ;HP
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB1103C ;HP_Alvorix
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB4103C ;HP_Inverness
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AB7103C ;HP_Apricot
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2ABA103C ;HP
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2ABC103C ;HP_Arrowwood
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2ABD103C ;HP
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AC2103C ;HP_Carmel2
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AC6103C ;HP_Arroyo
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AC7103C ;HP_Armand
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2ACA103C ;HP
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AD0103C ;HP_Arrowwwod-E
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AD2103C ;HP_PauBrazil2
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AD6103C ;HP_Lawrence
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2ADF103C ;HP_Brabus
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AE8103C ;HP_Brabus2
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AE9103C ;HP_Armand2
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AEB103C ;HP_Lowrence2
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AEF103C ;HP
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AF0103C ;HP_Ambu
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AF1103C ;HP_Loom
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AF2103C ;HP_Arroyo3
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2AF5103C ;HP_Armand3
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_2B00103C ;HP_Arroyo4
%RTL8136.DeviceDesc% = RTL8105S5WOLDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_357F103C ;HP_SMART

; 8105E S5 WOL Hide and Default Enable
%RTL8136.DeviceDesc% = RTL8105S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1584103C&REV_05 ;HP
%RTL8136.DeviceDesc% = RTL8105S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1585103C&REV_05 ;HP
%RTL8136.DeviceDesc% = RTL8105S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1676103C&REV_05 ;HP
%RTL8136.DeviceDesc% = RTL8105S5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1678103C&REV_05 ;HP

; 8105E S5 WOL Hide and Default Disable
%RTL8136.DeviceDesc% = RTL8105S5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_1586103C&REV_05 ;HP

; 8105E EEE Default Enable
%RTL8136.DeviceDesc% = RTL8105EEEEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_162A10CF&REV_05 ;Fuji
%RTL8136.DeviceDesc% = RTL8105EEEEnable.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_175B10CF&REV_05 ;Fuji


; 8402
%RTL8136.DeviceDesc% = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&REV_06


; 8168F
%RTL8168.DeviceDesc% = RTL8168F.ndi, PCI\VEN_10EC&DEV_8168&REV_07

; 8168F S5 WOL Hide and Default Enable
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17EA103C&REV_07 ;HP_Popeye(UMA)
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17EB103C&REV_07 ;HP_Popeye(DSC)
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17ED103C&REV_07 ;HP_Pebbles(UMA)
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17EE103C&REV_07 ;HP_Pebbles(DSC)
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17F0103C&REV_07 ;HP_Richie(UMA)
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17F1103C&REV_07 ;HP_Richie(DSC)
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17F3103C&REV_07 ;HP_Roadrunner
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17F4103C&REV_07 ;HP_Rocky(DSC)
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_17F6103C&REV_07 ;HP_Rocky(UMA)
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_180E103C&REV_07 ;HP_Tarzan
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_180F103C&REV_07 ;HP_Tarzan
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1810103C&REV_07 ;HP_Tigger
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideEnable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_1846103C&REV_07 ;HP_Roger(UMA)

; 8168F S5 WOL Hide and Default Disable
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9095104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9096104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9099104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_909B104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90A5104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90A6104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90AA104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90AB104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90AD104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90AF104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90B0104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90A8104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLHideDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_90AC104D&REV_07 ;SONY

; 8168F S5 WOL Default Disable
%RTL8168.DeviceDesc% = RTL8168FS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ADA103C ;HP
%RTL8168.DeviceDesc% = RTL8168FS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2ADF103C ;HP_Brabus
%RTL8168.DeviceDesc% = RTL8168FS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AE8103C ;HP_Brabus2
%RTL8168.DeviceDesc% = RTL8168FS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AE9103C ;HP_Armand2
%RTL8168.DeviceDesc% = RTL8168FS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AEF103C ;HP
%RTL8168.DeviceDesc% = RTL8168FS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2AF1103C ;HP_Loom
%RTL8168.DeviceDesc% = RTL8168FS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_9097104D&REV_07 ;SONY
%RTL8168.DeviceDesc% = RTL8168FS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_221917AA&REV_07 ;Lenovo
%RTL8168.DeviceDesc% = RTL8168FS5WOLDisable.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_510C17AA&REV_07 ;Lenovo

; 8168F EEE & Flow control Default Disable
%RTL8168.DeviceDesc% = RTL8168FEEEDnFCDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_600A17AA&REV_07 ;NEC
%RTL8168.DeviceDesc% = RTL8168FEEEDnFCDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_601917AA&REV_07 ;NEC
%RTL8168.DeviceDesc% = RTL8168FEEEDnFCDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_601C17AA&REV_07 ;NEC
%RTL8168.DeviceDesc% = RTL8168FEEEDnFCDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_604617AA&REV_07 ;NEC
%RTL8168.DeviceDesc% = RTL8168FEEEDnFCDn.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_A03F1BCF&REV_07 ;NEC


; 8168FB
%RTL8168.DeviceDesc% = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&REV_09

; 8168FR
%RTL8168.DeviceDesc% = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&REV_0B


; 8411
%RTL8168.DeviceDesc% = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&REV_0A


; 8166
%RTL8168.DeviceDesc% = RTL8168.ndi, PCI\VEN_10EC&DEV_8166


; 8118
%RTL8118.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_16
%RTL8118.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_17
%RTL8118.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_20
%RTL8118.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_25
%RTL8118.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_26

; E2500
%E2500.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_2502&REV_1F

; E2600
%E2600.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_2600&REV_21


; 8119
%RTL8168.DeviceDesc% = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&REV_18

; 8119i
%RTL8168.DeviceDesc% = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&REV_19


; 8125
%RTL8125.DeviceDesc%  = RTL8125.ndi, PCI\VEN_10EC&DEV_8125&REV_00
%RTL8125.DeviceDesc%  = RTL8125.ndi, PCI\VEN_10EC&DEV_8225&REV_00 ;Add-on card

; 8125AG
%RTL8125AG.DeviceDesc%  = RTL8125.ndi, PCI\VEN_10EC&DEV_8125&REV_01
%ASUS8125AG.DeviceDesc% = RTL8125.ndi,, PCI\VEN_10EC&DEV_8125&SUBSYS_18D20B05&REV_01 ;ASUS

; 8125AP
%RTL8125.DeviceDesc%  = RTL8125.ndi, PCI\VEN_10EC&DEV_8125&REV_02

; E3000
%E3000.DeviceDesc% = RTL8125.ndi, PCI\VEN_10EC&DEV_3000&REV_03


; Add-on card
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8161&REV_06
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8161&REV_0C
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8161&REV_15


; 8168F's successor
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_0C
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_0D
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_0E
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_0F
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_10
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_11
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_12
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_13
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_14
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_15
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_1A
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_1B
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_1C
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_1D
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_1E
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_1F
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_21
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_22
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_23
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_24
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_27
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_28
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_29
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_2A
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_2B
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_2C
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_2D
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_2E
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_30
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_31
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_32
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_33
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_34
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_35
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_36
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_37
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_38
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_39
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_3A
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_3B
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_3C
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_3D
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_3E
%RTL8168.DeviceDesc% = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_3F


; 8105E's successor
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_07
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_08
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_09
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_0A
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_0B
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_0C
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_0D
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_0E
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_0F
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_10
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_11
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_12
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_13
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_14
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_15
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_16
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_17
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_18
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_19
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1A
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1B
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1C
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1D
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1E
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1F
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_20
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_21
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_22
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_23
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_24
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_25
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_26
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_27
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_28
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_29
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_2A
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_2B
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_2C
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_2D
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_2E
%RTL8136.DeviceDesc% = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_2F


; 8125's successor
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_03
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_03
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_04
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_04
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_05
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_05
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_06
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_06
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_07
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_07
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_08
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_08
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_09
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_09
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_0A
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_0A
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_0B
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_0B
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_0C
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_0C
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_0D
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_0D
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_0E
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_0E
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_0F
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_0F
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_10
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_10
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_11
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_11
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_12
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_12
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_13
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_13
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_14
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_14
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_15
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_15
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_16
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_16
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_17
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_17
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_18
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_18
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_19
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_19
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_1A
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_1A
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_1B
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_1B
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_1C
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_1C
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_1D
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_1D
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_1E
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_1E
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&REV_1F
%RTL8125.DeviceDesc%  = RTL8125Series.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_1F


; Realtek
;
; Windows NT specific entry

[R8169C7k.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, JumboNolimit.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8169.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, Jumboframe.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, Jumboframe4k.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168Series.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = rtk.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8136.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8136Series.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = rtk.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8136HP.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
AddReg          = AutoCrossoverDet.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8136HPS5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, s5woldefaultdisable.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
AddReg          = AutoCrossoverDet.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168C.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168CS5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5woldefaultdisable.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168CNotSpdDown.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolS5LinkSpeedNotSpdDown.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168CForceGigabit.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed1g.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolS5LinkSpeedForce1g.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168CForce100Full.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = SpeedForce100Full.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8102.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8102S5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5woldefaultdisable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8102S5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wolhideenable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8102ForceEnableClkReq.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168D.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168DS5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5woldefaultdisable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168DS5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhideenable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168DP.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168E.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168ES5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5woldefaultdisable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168ES5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhideenable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168EEEEEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168EEEEEnS5WOLHideDn.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhidedisable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168EEEEDnFCDn.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrlDisable.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168ES.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168F.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168FS5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168FS5WOLHideDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhidedisable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168FS5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5woldefaultdisable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168FEEEDnFCDn.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrlDisable.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8168FB.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8125.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed2.5G.reg, NetworkAddress.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf8125.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8125Series.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed2.5G.reg, NetworkAddress.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = rtk.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8104.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg
AddReg          = WolShutdownLinkSpeed.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8105.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8105S5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5woldefaultdisable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8105S5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wolhideenable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8105S5WOLHideDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wolhidedisable.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[RTL8105EEEEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3


[RTL8168.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168Series.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8136.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8136Series.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8136HP.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8136HPS5WOLDisable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168C.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168CS5WOLDisable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168CNotSpdDown.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168CForceGigabit.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168CForce100Full.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8102.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8102S5WOLDisable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8102S5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8102ForceEnableClkReq.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168D.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168DS5WOLDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168DS5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168DP.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168E.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168ES5WOLDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168ES5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168EEEEEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168EEEEEnS5WOLHideDn.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168EEEEDnFCDn.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168ES.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168F.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FS5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FS5WOLHideDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FS5WOLDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FEEEDnFCDn.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FB.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8125.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8125Series.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8104.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8105.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8105S5WOLDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8105S5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8105S5WOLHideDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8105EEEEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW


[RTL8168_8136.MSI.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

[RTL8168D.MSI.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1


[R8169C7k.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8169.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168Series.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8136.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8136Series.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8136HP.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8136HPS5WOLDisable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168C.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168CS5WOLDisable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168CNotSpdDown.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168CForceGigabit.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168CForce100Full.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8102.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8102S5WOLDisable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8102S5WOLHideEnable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8102ForceEnableClkReq.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168D.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168DS5WOLDisable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168DS5WOLHideEnable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168DP.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168E.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168ES5WOLDisable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168ES5WOLHideEnable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168EEEEEnable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168EEEEEnS5WOLHideDn.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168EEEEDnFCDn.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168ES.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168F.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168FS5WOLHideEnable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168FS5WOLHideDisable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168FS5WOLDisable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168FEEEDnFCDn.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8168FB.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8125.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8125Series.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8104.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8105.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8105S5WOLDisable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8105S5WOLHideEnable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8105S5WOLHideDisable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog

[RTL8105EEEEnable.ndi.NT.Services]
AddService = rt640x64, 2, rt640.Service, common.EventLog



;-----------------------------------------------------------------------------
; common base for 10/100/1000 Mb Adapters
;
[Speed.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

[Speed1g.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "6"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"6"

HKR,,ForceMode,0,"0"

[Speed10_100.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

[SpeedForce100Full.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"4"

HKR,,ForceMode,0,"1"

[Speed2.5G.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2500",     0, %2.5Gb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

[NetworkAddress.reg]
HKR,Ndi\params\NetworkAddress,	   ParamDesc,  0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,	   type,       0, "edit"
HKR,Ndi\params\NetworkAddress,	   default,    0, ""
HKR,Ndi\params\NetworkAddress,	   LimitText,  0, "12"
HKR,Ndi\params\NetworkAddress,	   UpperCase,  0, "1"
HKR,Ndi\params\NetworkAddress,	   Optional,   0, "1"

[flowctrl.reg]
HKR,Ndi\params\*FlowControl,	   ParamDesc,  0, %FlowControl%
HKR,Ndi\params\*FlowControl,	   default,    0, "3"
HKR,Ndi\params\*FlowControl,	   type,       0, "enum"
HKR,Ndi\params\*FlowControl\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*FlowControl\enum,  "3",        0, %RxTxEnabled%
HKR,,*FlowControl,0,"3"

[flowctrlDisable.reg]
HKR,Ndi\params\*FlowControl,       ParamDesc,  0, %FlowControl%
HKR,Ndi\params\*FlowControl,       default,    0, "0"
HKR,Ndi\params\*FlowControl,       type,       0, "enum"
HKR,Ndi\params\*FlowControl\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*FlowControl\enum,  "3",        0, %RxTxEnabled%
HKR,,*FlowControl,0,"0"

[PriorityVlanTag.reg]
HKR,Ndi\params\*PriorityVLANTag,	ParamDesc,  0, %PriorityVLAN%
HKR,Ndi\params\*PriorityVLANTag,	default,    0, "3"
HKR,Ndi\params\*PriorityVLANTag,	type,       0, "enum"
HKR,Ndi\params\*PriorityVLANTag\enum,	"0",        0, %PriorityVLANDisabled%
HKR,Ndi\params\*PriorityVLANTag\enum,	"1",        0, %PriorityEnabled%
HKR,Ndi\params\*PriorityVLANTag\enum,	"2",        0, %VLANEnabled%
HKR,Ndi\params\*PriorityVLANTag\enum,	"3",        0, %PriorityVLANEnabled%
HKR,,*PriorityVLANTag,0,"3"

[InterruptModeration.reg]
HKR,Ndi\params\*InterruptModeration,	ParamDesc,  0, %InterruptModeration%
HKR,Ndi\params\*InterruptModeration,	default,    0, "1"
HKR,Ndi\params\*InterruptModeration,	type,       0, "enum"
HKR,Ndi\params\*InterruptModeration\enum,	"0",        0, %Disabled%
HKR,Ndi\params\*InterruptModeration\enum,	"1",        0, %Enabled%
HKR,,*InterruptModeration,0,"1"

[TxRxBuf.reg]
HKR,Ndi\Params\*ReceiveBuffers,       ParamDesc,  0, %ReceiveBuffers%
HKR,Ndi\Params\*ReceiveBuffers,       Type,       0, "int"
HKR,Ndi\Params\*ReceiveBuffers,       Default,    0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Min,        0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Max,        0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Step,       0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Base,       0, "10"
HKR,,*ReceiveBuffers,0,"512"

HKR,Ndi\Params\*TransmitBuffers,      ParamDesc,  0, %TransmitBuffers%
HKR,Ndi\Params\*TransmitBuffers,      Type,       0, "int"
HKR,Ndi\Params\*TransmitBuffers,      Default,    0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Min,        0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Max,        0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Step,       0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Base,       0, "10"
HKR,,*TransmitBuffers,0,"128"

[TxRxBuf8125.reg]
HKR,Ndi\Params\*ReceiveBuffers,       ParamDesc,  0, %ReceiveBuffers%
HKR,Ndi\Params\*ReceiveBuffers,       Type,       0, "int"
HKR,Ndi\Params\*ReceiveBuffers,       Default,    0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Min,        0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Max,        0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Step,       0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Base,       0, "10"
HKR,,*ReceiveBuffers,0,"512"

HKR,Ndi\Params\*TransmitBuffers,      ParamDesc,  0, %TransmitBuffers%
HKR,Ndi\Params\*TransmitBuffers,      Type,       0, "int"
HKR,Ndi\Params\*TransmitBuffers,      Default,    0, "512"
HKR,Ndi\Params\*TransmitBuffers,      Min,        0, "64"
HKR,Ndi\Params\*TransmitBuffers,      Max,        0, "4096"
HKR,Ndi\Params\*TransmitBuffers,      Step,       0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Base,       0, "10"
HKR,,*TransmitBuffers,0,"512"

[Jumboframe.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,,*JumboPacket,0,"1514"

[Jumboframe4k.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,,*JumboPacket,0,"1514"

[Jumboframe9k.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "8192",     0, %8KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "9216",     0, %9KBMTU%
HKR,,*JumboPacket,0,"1514"

[JumboNolimit.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,,*JumboPacket,0,"1514"
HKR,,LimitCbJumboFrame,0,"0"

[Offload.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*LsoV1IPv4,	ParamDesc,  0, %LSOv4%
HKR,Ndi\params\*LsoV1IPv4,	default,    0, "1"
HKR,Ndi\params\*LsoV1IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV1IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV1IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV1IPv4,0,"1"

[OffloadChksum.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

[s5wol.reg]
HKR,,S5WakeOnLan,0,"1"

[s5woldefaultdisable.reg]
HKR,,S5WakeOnLan,0,"0"

[s5wolhideenable.reg]
HKR,,S5WakeOnLan,0,"1"

[s5wolhidedisable.reg]
HKR,,S5WakeOnLan,0,"0"

[OffloadIpv6Lsov2.reg]
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       ParamDesc,  0, %TCPChksumOffv6%
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv6,       ParamDesc,  0, %UDPChksumOffv6%
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*LsoV2IPv4,	ParamDesc,  0, %LSOv2v4%
HKR,Ndi\params\*LsoV2IPv4,	default,    0, "0"
HKR,Ndi\params\*LsoV2IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv4,0,"0"

HKR,Ndi\params\*LsoV2IPv6,	ParamDesc,  0, %LSOv2v6%
HKR,Ndi\params\*LsoV2IPv6,	default,    0, "1"
HKR,Ndi\params\*LsoV2IPv6,	type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv6\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv6,0,"1"

HKR,Ndi\params\*LsoV1IPv4,	ParamDesc,  0, %LSOv4%
HKR,Ndi\params\*LsoV1IPv4,	default,    0, "1"
HKR,Ndi\params\*LsoV1IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV1IPv4\enum,  "0",       0, %Disabled%
HKR,Ndi\params\*LsoV1IPv4\enum,  "1",       0, %Enabled%
HKR,,*LsoV1IPv4,0,"1"

[OffloadIpv6Lsov2_8102.reg]
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       ParamDesc,  0, %TCPChksumOffv6%
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv6,       ParamDesc,  0, %UDPChksumOffv6%
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*LsoV2IPv4,	ParamDesc,  0, %LSOv2v4%
HKR,Ndi\params\*LsoV2IPv4,	default,    0, "1"
HKR,Ndi\params\*LsoV2IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv4,0,"1"

HKR,Ndi\params\*LsoV2IPv6,	ParamDesc,  0, %LSOv2v6%
HKR,Ndi\params\*LsoV2IPv6,	default,    0, "1"
HKR,Ndi\params\*LsoV2IPv6,	type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv6\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv6,0,"1"

[AutoCrossoverDet.reg]
HKR,Ndi\params\AutoCrossoverDet,	ParamDesc,  0, %AutoCrossoverDet%
HKR,Ndi\params\AutoCrossoverDet,	default,    0, "0"
HKR,Ndi\params\AutoCrossoverDet,	type,       0, "enum"
HKR,Ndi\params\AutoCrossoverDet\enum,   "0",        0, %Disabled%
HKR,Ndi\params\AutoCrossoverDet\enum,   "1",        0, %Enabled%
HKR,,AutoCrossoverDet,0,"0"

[WolShutdownLinkSpeed.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,	ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,	default,    0, "0"
HKR,Ndi\params\WolShutdownLinkSpeed,	type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "0",    0, %10MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "1",    0, %100MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"0"

[WolS5LinkSpeedNotSpdDown.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,	ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,	default,    0, "2"
HKR,Ndi\params\WolShutdownLinkSpeed,	type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "0",    0, %10MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "1",    0, %100MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[WolS5LinkSpeedForce1g.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,	ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,	default,    0, "2"
HKR,Ndi\params\WolShutdownLinkSpeed,	type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[wolptnmagic.reg]
HKR,Ndi\params\*WakeOnPattern,  ParamDesc,  0, %WakeOnPtn%
HKR,Ndi\params\*WakeOnPattern,	default,    0, "1"
HKR,Ndi\params\*WakeOnPattern,	type,       0, "enum"
HKR,Ndi\params\*WakeOnPattern\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnPattern\enum,   "1",        0, %Enabled%
HKR,,*WakeOnPattern,0,"1"

HKR,Ndi\params\*WakeOnMagicPacket,	ParamDesc,  0, %WakeOnMagPkt%
HKR,Ndi\params\*WakeOnMagicPacket,	default,    0, "1"
HKR,Ndi\params\*WakeOnMagicPacket,	type,       0, "enum"
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "1",        0, %Enabled%
HKR,,*WakeOnMagicPacket,0,"1"

[ArpNsProtOffload.reg]
HKR,Ndi\params\*PMARPOffload,       ParamDesc,  0, %ArpOffload%
HKR,Ndi\params\*PMARPOffload,	    default,    0, "1"
HKR,Ndi\params\*PMARPOffload,	    type,       0, "enum"
HKR,Ndi\params\*PMARPOffload\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*PMARPOffload\enum,  "1",        0, %Enabled%
HKR,,*PMARPOffload,0,"1"

HKR,Ndi\params\*PMNSOffload,	    ParamDesc,  0, %NsOffload%
HKR,Ndi\params\*PMNSOffload,	    default,    0, "1"
HKR,Ndi\params\*PMNSOffload,	    type,       0, "enum"
HKR,Ndi\params\*PMNSOffload\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*PMNSOffload\enum,   "1",        0, %Enabled%
HKR,,*PMNSOffload,0,"1"


[del.reg]
HKR,Ndi\params

HKR,,*SpeedDuplex
HKR,,NetworkAddress
HKR,,*FlowControl
HKR,,*PriorityVLANTag
HKR,,*InterruptModeration
HKR,,*ReceiveBuffers
HKR,,*TransmitBuffers
HKR,,*JumboPacket
HKR,,*TCPChecksumOffloadIPv4
HKR,,*TCPChecksumOffloadIPv6
HKR,,*UDPChecksumOffloadIPv4
HKR,,*UDPChecksumOffloadIPv6
HKR,,*IPChecksumOffloadIPv4
HKR,,*LsoV1IPv4
HKR,,*LsoV2IPv4
HKR,,*LsoV2IPv6
HKR,,*RSS
HKR,,*NumRssQueues
HKR,,*WakeOnPattern
HKR,,*WakeOnMagicPacket
HKR,,*PMARPOffload
HKR,,*PMNSOffload
HKR,,*SelectiveSuspend
HKR,,*SSIdleTimeout
HKR,,*EEE
HKR,,EEE
HKR,,*HeaderDataSplit
HKR,,AutoCrossoverDet
HKR,,S5WakeOnLan
HKR,,S5ARPOffload
HKR,,WolShutdownLinkSpeed
HKR,,AutoDisableGigabit
HKR,,AutoLinkDownPcieMacOff
HKR,,ForceMode
HKR,,EnableGreenEthernet
HKR,,AdvancedEEE
HKR,,GigaLite
HKR,,WakeOnLinkUp
HKR,,DisablePBA
HKR,,PowerDownPll
HKR,,ForceEnableClkReq
HKR,,PPSW
HKR,,GPPSW
HKR,,AIPSMode
HKR,,JumboFrame
HKR,,S3S4WolPowerSaving
HKR,,WolCap
HKR,,S0MgcPkt
HKR,,LimitCbJumboFrame

[DMAr.reg]
HKR,Parameters,DmaRemappingCompatible,0x00010001,2
;1 = opt-in, 2 = opt-in only for external devices


;-----------------------------------------------------------------------------
; rtk NT specific
;

[rtk.reg]
HKR, Ndi,                       Service,    0, "rt640x64"
; use ndis5 as the upper bound because NT supports it
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"


[rt640.Service]
DisplayName     = %rt640.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\rt640x64.sys
LoadOrderGroup  = NDIS
AddReg          = DMAr.reg


[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\rt640x64.sys"
HKR, , TypesSupported,   0x00010001, 7

;-----------------------------------------------------------------------------
; DestinationDirs
;
[rt640.CopyFiles]
rt640x64.sys,,,2

[SourceDisksNames]
1 = %DiskDescription%


[SourceDisksFiles]
rt640x64.sys = 1,, ; on distribution disk 1


[DestinationDirs]
rt640.CopyFiles  = 12
DefaultDestDir     = 11

[Strings]
Realtek                  = "Realtek"
MSFT                     = "Microsoft"
AutoDetect               = "Auto Negotiation"
SpeedDuplex              = "Speed & Duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Network Address"
IPChksumOffv4            = "IPv4 Checksum Offload"
TCPChksumOffv4           = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4           = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6           = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6           = "UDP Checksum Offload (IPv6)"
Enabled                  = "Enabled"
Disabled                 = "Disabled"
TxEnabled                = "Tx Enabled"
RxEnabled                = "Rx Enabled"
RxTxEnabled              = "Rx & Tx Enabled"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Flow Control"
PriorityVLAN             = "Priority & VLAN"
PriorityVLANDisabled     = "Priority & VLAN Disabled"
PriorityVLANEnabled      = "Priority & VLAN Enabled"
InterruptModeration      = "Interrupt Moderation"
ReceiveBuffers           = "Receive Buffers"
TransmitBuffers          = "Transmit Buffers"
AutoDisableGigabit       = "Auto Disable Gigabit"
AutoLinkDownPhyOff       = "Auto Disable PHY"
BatteryRe-Link           = "Re-Link, Battery"
AcBatteryRe-Link         = "Re-Link, Battery or AC"
Battery                  = "Enabled, Battery"
AcBattery                = "Enabled, Battery or AC"
JumboFrame               = "Jumbo Frame"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Auto Disable PCIe"
RSS                      = "Receive Side Scaling"
AutoCrossoverDet         = "Auto Crossover Detection"
PriorityEnabled          = "Priority Enabled"
VLANEnabled              = "VLAN Enabled"
10MbFirst                = "10 Mbps First"
100MbFirst               = "100 Mbps First"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy-Efficient Ethernet"
HDSplit                  = "Header Data Split"
WakeOnLinkUp             = "Wake On Link Up"
NumRssQueues             = "Maximum Number of RSS Queues"
1Queue                   = "1 Queue"
2Queue                   = "2 Queues"
4Queue                   = "4 Queues"
IPSecv2                  = "IPsec Offload"
AH                       = "Auth Header Enabled"
ESP                      = "ESP Enabled"
AHESP                    = "Auth Header & ESP Enabled"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"

RTL8169.DeviceDesc       = "Realtek PCI GbE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"


SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"
LGSITV.DeviceDesc        = "LG System Interface(TV)"
TPLINKPCIEGBE.DeviceDesc = "TP-Link Gigabit PCI Express Adapter"
E2500.DeviceDesc         = "Killer E2500 Gigabit Ethernet Controller"
E2600.DeviceDesc         = "Killer E2600 Gigabit Ethernet Controller"
E3000.DeviceDesc         = "Killer E3000 2.5 Gigabit Ethernet Controller"
ASUS8125AG.DeviceDesc    = "ASUS 2.5G PCI-E Network Adapter"

rt640.Service.DispName = "Realtek RT640 NT Driver"

DiskDescription      = "Realtek Driver Disk 1"
