; Copyright (c) Microsoft Corporation.  All rights reserved.

[Version]
Signature="$WINDOWS NT$"
Class=System
ClassGuid={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%MSFT%
PnpLockdown=1
DriverVer = 06/21/2006,10.0.19041.1387

[SourceDisksNames]
3426=windows cd

[SourceDisksFiles]
pci.sys = 3426

[DestinationDirs]
DefaultDestDir = 12                ; DIRID_DRIVERS

[ControlFlags]
BasicDriverOk=*
ExcludeFromSelect=*

[Manufacturer]
%GENDEV_MFG%=GENDEV_SYS,NTamd64

[GENDEV_SYS.NTamd64]
%*PNP0A03.DeviceDesc%          = PCI_ROOT, *PNP0A03            ; ROOT PCI BUS
%*PNP0A08.DeviceDesc%          = PCI_ROOT, *PNP0A08            ; PCI Express Root Complex
%PCI\CC_0604.DeviceDesc%       = PCI_BRIDGE, PCI\CC_0604       ; PCI-PCI BRIDGE
%PCI\CC_0604&DT_4.DeviceDesc%  = PCI_BRIDGE, PCI\CC_0604&DT_4  ; PCI Express Root Port
%PCI\CC_0604&DT_5.DeviceDesc%  = PCI_BRIDGE, PCI\CC_0604&DT_5  ; PCI Express Upstream Switch Port
%PCI\CC_0604&DT_6.DeviceDesc%  = PCI_BRIDGE, PCI\CC_0604&DT_6  ; PCI Express Downstream Switch Port
%PCI\CC_0604&DT_7.DeviceDesc%  = PCI_BRIDGE, PCI\CC_0604&DT_7  ; PCI Express to PCI(-X) Bridge
%PCI\CC_0604&DT_8.DeviceDesc%  = PCI_BRIDGE, PCI\CC_0604&DT_8  ; PCI(-X) to PCI Express Bridge

;****************************************************
; PCI settings used externally by PCI device INFs via Include/Needs.
; See below for more information on usage.
;
%PCI.SettingDesc% = PciIoSpaceNotRequired
%PCI.SettingDesc% = PciSriovSupported
%PCI.SettingDesc% = PciAcsNotRequired
%PCI.SettingDesc% = PciASPMOptIn
%PCI.SettingDesc% = PciASPMOptOut
%PCI.SettingDesc% = PciD3ColdSupported
%PCI.SettingDesc% = PciDoNotUseAcs
%PCI.SettingDesc% = PciEnableAllBridgeInterrupts
%PCI.SettingDesc% = PciAtomicsOptIn
%PCI.SettingDesc% = PciExtraSettleTimeRequired
%PCI.SettingDesc% = PciIgnoreErrorsDuringPLDR
%PCI.SettingDesc% = PciForceSBR
%PCI.SettingDesc% = PciBridgeUseNativeWakeInfo

;****************************************************
; Generic PCI Root Bus/PCI-PCI Bridge
[PCI_ROOT]
CopyFiles=PCI_COPYFILES
AddReg = PCI_ROOT_REG

[PCI_COPYFILES]
pci.sys,,,0x100 ;COPYFLG_PROTECTED_WINDOWS_DRIVER_FILE

[PCI_ROOT.Services]
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection

[PCI_ROOT.HW]
AddReg = PCI_BRIDGE_HW.AddReg

[PCI_ROOT_REG]
HKR,,ResourcePickerExceptions,0,"IO:HAL,MBRES;MEM:HAL,MBRES"
HKR,,ResourcePickerTags,0,"MBRES"

[PCI_BRIDGE]
CopyFiles=PCI_COPYFILES

[PCI_BRIDGE.Services]
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection

[pci_ServiceInstallSection]
DisplayName    = %pci_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\pci.sys
LoadOrderGroup = "Boot Bus Extender"
AddReg = pci_ServiceInstallSection_AddReg

[pci_ServiceInstallSection_AddReg]
HKR,,Tag,0x00010001,3
HKR,Parameters,DmaRemappingCompatible,0x00010001,2

[PCI_BRIDGE.HW]
AddReg = PCI_BRIDGE_HW.AddReg

[PCI_BRIDGE_HW.AddReg]
HKR,,UINumberDescFormat,,%PCISlot%

;**************************************************************************
; Section for device INFs to include in their DDInstall section, for features
; that are not detectable by just looking at the device hardware.
; 
; Example INF usage for PCI-based device:
;
; [PciDevice_Install]
; ...
;
; [PciDevice_Install.HW]
; Include = pci.inf
; Needs   = PciIoSpaceNotRequired.HW, PciSriovSupported.HW
; ...
;
; Sections duplicated in machine.inf to maintain compatability with legacy INFs.
;

; IO space not required.
[PciIoSpaceNotRequired]
Needs=PciIoSpaceNotRequired.HW

[PciIoSpaceNotRequired.HW]
AddReg=PciIoSpaceNotRequired.RegHW

[PciIoSpaceNotRequired.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7,IoNotRequired,0x10001,1

; SRIOV supported.
[PciSriovSupported]
Needs=PciSriovSupported.HW

[PciSriovSupported.HW]
AddReg=PciSriovSupported.RegHW

[PciSriovSupported.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7,SriovSupported,0x10001,1

; ACS not required.
[PciAcsNotRequired]
Needs=PciAcsNotRequired.HW

[PciAcsNotRequired.HW]
AddReg=PciAcsNotRequired.RegHW

[PciAcsNotRequired.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7,AcsNotRequired,0x10001,1

; Opt-in to ASPM.
[PciASPMOptIn]
Needs=PciASPMOptIn.HW

[PciASPMOptIn.HW]
AddReg=PciASPMOptIn.RegHW

[PciASPMOptIn.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7,ASPMOptIn,0x10001,1

; Opt-out of ASPM.
[PciASPMOptOut]
Needs=PciASPMOptOut.HW

[PciASPMOptOut.HW]
AddReg=PciASPMOptOut.RegHW

[PciASPMOptOut.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7,ASPMOptOut,0x10001,1

; D3 cold supported.
[PciD3ColdSupported]
Needs=PciD3ColdSupported.HW

[PciD3ColdSupported.HW]
AddReg=PciD3ColdSupported.RegHW

[PciD3ColdSupported.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7,D3ColdSupported,0x10001,1

; Prevents Windows from enabling ACS on the Bridge.  Will also prevent
; any feature that requires ACS.
[PciDoNotUseAcs]
Needs=PciDoNotUseAcs.HW

[PciDoNotUseAcs.HW]
AddReg=PciDoNotUseAcs.RegHW

[PciDoNotUseAcs.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7,DoNotUseAcs,0x10001,1

; Normally Windows will filter out bridge interrupts that it does not use.
; Set this flag to disable bridge interrupt filtering.
[PciEnableAllBridgeInterrupts]
Needs=PciEnableAllBridgeInterrupts.HW

[PciEnableAllBridgeInterrupts.HW]
AddReg= PciEnableAllBridgeInterrupts.RegHW

[PciEnableAllBridgeInterrupts.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7, EnableAllBridgeInterrupts,0x10001,1

; Opt-in to Atomics.
[PciAtomicsOptIn]
Needs=PciAtomicsOptIn.HW

[PciAtomicsOptIn.HW]
AddReg=PciAtomicsOptIn.RegHW

[PciAtomicsOptIn.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7,AtomicsOptIn,0x10001,1

; Set this flag if a device requires extra
; settle time after D3Cold transitions.
[PciExtraSettleTimeRequired]
Needs=PciExtraSettleTimeRequired.HW

[PciExtraSettleTimeRequired.HW]
AddReg=PciExtraSettleTimeRequired.RegHW

[PciExtraSettleTimeRequired.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7, SettleTimeRequired,0x10001,1

; Set this flag if a device generates
; errors that should be ignored during
; PLDR.
[PciIgnoreErrorsDuringPLDR]
Needs=PciIgnoreErrorsDuringPLDR.HW

[PciIgnoreErrorsDuringPLDR.HW]
AddReg=PciIgnoreErrorsDuringPLDR.RegHW

[PciIgnoreErrorsDuringPLDR.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7, IgnoreErrorsDuringPLDR,0x10001,1

; Set this flag if a device wants to force Secondary Bus Reset event if
; it has sibling functions.
[PciForceSBR]
Needs=PciForceSBR.HW

[PciForceSBR.HW]
AddReg=PciForceSBR.RegHW

[PciForceSBR.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7, ForceSBR,0x10001,1

; Set this flag if a non-root-integrated bridge wants to determine its lowest
; wake-able D-state in S0 from native PCI PMCSR register
[PciBridgeUseNativeWakeInfo]
Needs=PciBridgeUseNativeWakeInfo.HW

[PciBridgeUseNativeWakeInfo.HW]
AddReg=PciBridgeUseNativeWakeInfo.RegHW

[PciBridgeUseNativeWakeInfo.RegHW]
HKR,e5b3b5ac-9725-4f78-963f-03dfb1d828c7, BridgeUseNativeWakeInfo,0x10001,1

[Strings]
; localizable
MSFT            = "Microsoft"

;*******************************************
;device descriptions

GENDEV_MFG = "(Standard system devices)"
*pnp0a03.DeviceDesc           = "PCI Bus"
*pnp0a08.DeviceDesc           = "PCI Express Root Complex"
PCI\CC_0604.DeviceDesc        = "PCI-to-PCI Bridge"
PCI\CC_0604&DT_4.DeviceDesc   = "PCI Express Root Port"
PCI\CC_0604&DT_5.DeviceDesc   = "PCI Express Upstream Switch Port"
PCI\CC_0604&DT_6.DeviceDesc   = "PCI Express Downstream Switch Port"
PCI\CC_0604&DT_7.DeviceDesc   = "PCI Express to PCI/PCI-X Bridge"
PCI\CC_0604&DT_8.DeviceDesc   = "PCI/PCI-X to PCI Express Bridge"

;*******************************************
;setting descriptions
PCI.SettingDesc = "PCI Device Setting"

;*******************************************
PCISlot = "PCI Slot %1!u!"

;*******************************************
;service descriptions
pci_svcdesc = "PCI Bus Driver"

;*******************************************
;Non-localizable
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_DEMAND_START   = 3
SERVICE_ERROR_NORMAL   = 1
SERVICE_ERROR_CRITICAL = 3
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
