; Copyright (c) Microsoft Corporation.  All rights reserved.

[Version]
Signature="$WINDOWS NT$"
Class=hdc
ClassGuid={4D36E96A-E325-11CE-BFC1-08002BE10318}
Provider=%MS%
PnpLockdown=1
DriverVer = 06/21/2006,10.0.19041.1288

[SourceDisksNames]
3426=windows cd

[SourceDisksFiles]
storahci.sys = 3426
intelide.sys    = 3426
atapi.sys   = 3426
ataport.sys     = 3426
pciidex.sys     = 3426
pciide.sys  = 3426

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS

[ControlFlags]
BasicDriverOk=*
ExcludeFromSelect=*

[Manufacturer]
%MS-Drivers%=MS_HDC,NTamd64...0x01,NTamd64...0x02,NTamd64...0x03
%INTEL%=INTEL_HDC,NTamd64
%SIS%=SIS_HDC,NTamd64
%IBM%=IBM_HDC,NTamd64...0x01,NTamd64...0x02,NTamd64...0x03
%LEXAR%=LEXAR_HDC,NTamd64...0x01,NTamd64...0x02,NTamd64...0x03
%SONY%=SONY_HDC,NTamd64...0x01,NTamd64...0x02,NTamd64...0x03
%SERVERWORKS%=SERVERWORKS_HDC,NTamd64
%NVIDIA%=NVIDIA_HDC,NTamd64
%MS-AHCI%=AHCI_HDC, NTamd64...0x01, NTamd64...0x02, NTamd64...0x03

[MS_HDC.NTamd64...0x01]
%pcmcia.DeviceDesc%      = pcmcia_atapi_Inst, PCMCIA\*PNP0600  ; PCMCIA IDE Controller
%idechannel.DeviceDesc%  = atapi_Inst, Internal_IDE_Channel    ; IDE Channel
%idechannel.DeviceDesc%  = atapi_Inst, Primary_IDE_Channel     ; Primary IDE Channel
%idechannel.DeviceDesc%  = atapi_Inst, Secondary_IDE_Channel   ; Secondary IDE Channel
%PCI\CC_0101.DeviceDesc% = pciide_Inst, PCI\CC_0101            ; PCI IDE Controller

[MS_HDC.NTamd64...0x02]
%pcmcia.DeviceDesc%      = pcmcia_atapi_Inst_Server, PCMCIA\*PNP0600  ; PCMCIA IDE Controller
%idechannel.DeviceDesc%  = atapi_Inst_Server, Internal_IDE_Channel    ; IDE Channel
%idechannel.DeviceDesc%  = atapi_Inst_Server, Primary_IDE_Channel     ; Primary IDE Channel
%idechannel.DeviceDesc%  = atapi_Inst_Server, Secondary_IDE_Channel   ; Secondary IDE Channel
%PCI\CC_0101.DeviceDesc% = pciide_Inst, PCI\CC_0101                   ; PCI IDE Controller

[MS_HDC.NTamd64...0x03]
%pcmcia.DeviceDesc%      = pcmcia_atapi_Inst_Server, PCMCIA\*PNP0600  ; PCMCIA IDE Controller
%idechannel.DeviceDesc%  = atapi_Inst_Server, Internal_IDE_Channel    ; IDE Channel
%idechannel.DeviceDesc%  = atapi_Inst_Server, Primary_IDE_Channel     ; Primary IDE Channel
%idechannel.DeviceDesc%  = atapi_Inst_Server, Secondary_IDE_Channel   ; Secondary IDE Channel
%PCI\CC_0101.DeviceDesc% = pciide_Inst, PCI\CC_0101                   ; PCI IDE Controller

[INTEL_HDC.NTamd64]
%PCI\VEN_8086&DEV_1222.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_1222     ; Intel PIIX  
%PCI\VEN_8086&DEV_1230.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_1230     ; Intel PIIX  
%PCI\VEN_8086&DEV_7010.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_7010     ; Intel PIIX3 
%PCI\VEN_8086&DEV_7111.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_7111     ; Intel PIIX4 
%PCI\VEN_8086&DEV_2411.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_2411     ; Intel ICH   
%PCI\VEN_8086&DEV_2421.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_2421     ; Intel ICH-0 
%PCI\VEN_8086&DEV_244A.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_244A     ; Intel ICH-2 
%PCI\VEN_8086&DEV_244B.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_244B     ; Intel ICH-2 
%PCI\VEN_8086&DEV_248A.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_248A     ; Intel ICH-3 
%PCI\VEN_8086&DEV_248B.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_248B     ; Intel ICH-3 
%PCI\VEN_8086&DEV_24C1.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_24C1     ; Intel ICH-4 
%PCI\VEN_8086&DEV_24CA.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_24CA     ; Intel ICH-4 
%PCI\VEN_8086&DEV_24CB.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_24CB     ; Intel ICH-4 
%PCI\VEN_8086&DEV_24D1.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_24D1     ; Intel ICH-5 
%PCI\VEN_8086&DEV_24DB.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_24DB     ; Intel ICH-5 
%PCI\VEN_8086&DEV_25A2.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_25A2     ; Intel ICH-5 
%PCI\VEN_8086&DEV_25A3.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_25A3     ; Intel ICH-5
%PCI\VEN_8086&DEV_2651.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_2651&CC_0101  ; Intel ICH-6
%PCI\VEN_8086&DEV_2652.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_2652&CC_0101  ; Intel ICH-6
%PCI\VEN_8086&DEV_2653.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_2653&CC_0101  ; Intel ICH-6
%PCI\VEN_8086&DEV_266F.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_266F     ; Intel ICH-6 
%PCI\VEN_8086&DEV_7199.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_7199     ; Intel 7199  (SINGLE)
%PCI\VEN_8086&DEV_7601.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_7601     ; Intel 7601  (IA64)
%PCI\VEN_8086&DEV_27C0.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_27C0          ; Intel ICH7 
%PCI\VEN_8086&DEV_27C4.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_27C4          ; Intel ICH7-M    
%PCI\VEN_8086&DEV_27DF.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_27DF          ; Intel ICH7
%PCI\VEN_8086&DEV_2820.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_2820         ; Intel ICH8 4 port
%PCI\VEN_8086&DEV_2825.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_2825         ; Intel ICH8 2 port
%PCI\VEN_8086&DEV_2828.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_2828         ; Intel ICH8 3 port
%PCI\VEN_8086&DEV_2850.DeviceDesc%=intelide_Inst, PCI\VEN_8086&DEV_2850         ; Intel ICH8

[SIS_HDC.NTamd64]
%PCI\VEN_1039&DEV_0601.DeviceDesc%=pciide_Inst, PCI\VEN_1039&DEV_0601       ; 
%PCI\VEN_1039&DEV_5513.DeviceDesc%=pciide_Inst, PCI\VEN_1039&DEV_5513       ; 

[IBM_HDC.NTamd64...0x01]
%PCMCIA\IBM-MICRODRIVE-7F50.DeviceDesc%=pcmcia_atapi_Inst, PCMCIA\IBM-MICRODRIVE-7F50 ; IBM Micro Drive
%PCMCIA\IBM-MICRODRIVE-AA55.DeviceDesc%=pcmcia_atapi_Inst, PCMCIA\IBM-MICRODRIVE-AA55 ; IBM Micro Drive

[IBM_HDC.NTamd64...0x02]
%PCMCIA\IBM-MICRODRIVE-7F50.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\IBM-MICRODRIVE-7F50 ; IBM Micro Drive
%PCMCIA\IBM-MICRODRIVE-AA55.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\IBM-MICRODRIVE-AA55 ; IBM Micro Drive

[IBM_HDC.NTamd64...0x03]
%PCMCIA\IBM-MICRODRIVE-7F50.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\IBM-MICRODRIVE-7F50 ; IBM Micro Drive
%PCMCIA\IBM-MICRODRIVE-AA55.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\IBM-MICRODRIVE-AA55 ; IBM Micro Drive

[SERVERWORKS_HDC.NTamd64]
%PCI\VEN_1166&DEV_0211.DeviceDesc%=serverworks_Inst, PCI\VEN_1166&DEV_0211       
%PCI\VEN_1166&DEV_0212&SUBSYS_02121166.DeviceDesc%=serverworks_Inst, PCI\VEN_1166&DEV_0212&SUBSYS_02121166 

[LEXAR_HDC.NTamd64...0x01]
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-HURRIC_-172F
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-TIDALWV-0E97
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst, PCMCIA\____CL_ATA_FLASH_CARD_LEXAR__-HURRIC_-DC37
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-TORNADO-29EC
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-TIDALWV-FD21
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst, PCMCIA\LEXARMEDIA_ATA_FLASH_CARD-HUR_HP_-0623

[LEXAR_HDC.NTamd64...0x02]
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-HURRIC_-172F
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-TIDALWV-0E97
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\____CL_ATA_FLASH_CARD_LEXAR__-HURRIC_-DC37
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-TORNADO-29EC
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-TIDALWV-FD21
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\LEXARMEDIA_ATA_FLASH_CARD-HUR_HP_-0623

[LEXAR_HDC.NTamd64...0x03]
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-HURRIC_-172F
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-TIDALWV-0E97
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\____CL_ATA_FLASH_CARD_LEXAR__-HURRIC_-DC37
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-TORNADO-29EC
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\CL_ATA_FLASH_CARD_LEXAR__-TIDALWV-FD21
%LEXAR.DeviceDesc%=pcmcia_atapi_Inst_Server, PCMCIA\LEXARMEDIA_ATA_FLASH_CARD-HUR_HP_-0623

[SONY_HDC.NTamd64...0x01]
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst,PCMCIA\SONY-MEMORYSTICK(__4M)-E637
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst,PCMCIA\SONY-MEMORYSTICK(__8M)-9EB3
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst,PCMCIA\SONY-MEMORYSTICK(_16M)-D04D
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst,PCMCIA\SONY-MEMORYSTICK(_32M)-1766
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst,PCMCIA\SONY-MEMORYSTICK(_64M)-8C2C 

[SONY_HDC.NTamd64...0x02]
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst_Server,PCMCIA\SONY-MEMORYSTICK(__4M)-E637
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst_Server,PCMCIA\SONY-MEMORYSTICK(__8M)-9EB3
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst_Server,PCMCIA\SONY-MEMORYSTICK(_16M)-D04D
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst_Server,PCMCIA\SONY-MEMORYSTICK(_32M)-1766
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst_Server,PCMCIA\SONY-MEMORYSTICK(_64M)-8C2C 

[SONY_HDC.NTamd64...0x03]
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst_Server,PCMCIA\SONY-MEMORYSTICK(__4M)-E637
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst_Server,PCMCIA\SONY-MEMORYSTICK(__8M)-9EB3
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst_Server,PCMCIA\SONY-MEMORYSTICK(_16M)-D04D
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst_Server,PCMCIA\SONY-MEMORYSTICK(_32M)-1766
%PCMCIA\SONY-MEMORYSTICK.DeviceDesc%=pcmcia_atapi_Inst_Server,PCMCIA\SONY-MEMORYSTICK(_64M)-8C2C 

[NVIDIA_HDC.NTamd64]
%PCI\VEN_10DE&DEV_00E3.DeviceDesc%=pciide_Inst, PCI\VEN_10DE&DEV_00E3 ; NVIDIA
%PCI\VEN_10DE&DEV_00E5.DeviceDesc%=pciide_Inst, PCI\VEN_10DE&DEV_00E5 ; NVIDIA
%PCI\VEN_10DE&DEV_00EE.DeviceDesc%=pciide_Inst, PCI\VEN_10DE&DEV_00EE ; NVIDIA

; AHCI installation section for Workstation
[AHCI_HDC.NTamd64...0x01]
%PCI\CC_010601.DeviceDesc%=msahci_Inst, PCI\CC_010601; Standard SATA AHCI Controller
%ACPI\CLS_0001&SUBCLS_0006&PI_01.DeviceDesc% = msahci_Inst, ACPI\CLS_0001&SUBCLS_0006&PI_01

; AHCI installation section for Domain Controller
[AHCI_HDC.NTamd64...0x02]
%PCI\CC_010601.DeviceDesc%=msahci_Inst_Server, PCI\CC_010601; Standard SATA AHCI Controller
%ACPI\CLS_0001&SUBCLS_0006&PI_01.DeviceDesc% = msahci_Inst_Server, ACPI\CLS_0001&SUBCLS_0006&PI_01
%ACPI\AMDI0600.DeviceDesc% = msahci_Inst_Server, ACPI\AMDI0600 ; TODO Needs to be removed once we have final Firmware

; AHCI installation section for Server
[AHCI_HDC.NTamd64...0x03]
%PCI\CC_010601.DeviceDesc%=msahci_Inst_Server, PCI\CC_010601; Standard SATA AHCI Controller
%ACPI\CLS_0001&SUBCLS_0006&PI_01.DeviceDesc% = msahci_Inst_Server, ACPI\CLS_0001&SUBCLS_0006&PI_01
%ACPI\AMDI0600.DeviceDesc% = msahci_Inst_Server, ACPI\AMDI0600 ; TODO Needs to be removed once we have final Firmware

[atapi_copyfiles]
atapi.sys,,,0x100
ataport.sys,,,0x100

[pciidex_copyfiles]
pciidex.sys,,,0x100
atapi.sys,,,0x100
ataport.sys,,,0x100

;*******************************************************
; Channel driver (atapi.sys) for pcmcia ide controllers
[pcmcia_atapi_Inst]
CopyFiles = atapi_copyfiles
AddReg = atapi_property_provider_AddReg

[pcmcia_atapi_Inst_Server]
CopyFiles = atapi_copyfiles
AddReg = atapi_property_provider_AddReg

[pcmcia_atapi_Inst.Services]
AddService = atapi, %SPSVCINST_ASSOCSERVICE%, atapi_Service_Inst, atapi_EventLog_Inst

[pcmcia_atapi_Inst_Server.Services]
AddService = atapi, %SPSVCINST_ASSOCSERVICE%, atapi_Service_Inst_Server, atapi_EventLog_Inst

[pcmcia_atapi_Inst.HW]
AddReg = atapi_interrupt_priority_AddReg

[pcmcia_atapi_Inst_Server.HW]
AddReg = atapi_interrupt_priority_AddReg

;****************************************************
; Channel driver (atapi.sys) for pci ide controllers
[atapi_Inst]
CopyFiles = atapi_copyfiles
AddReg = atapi_property_provider_AddReg

[atapi_Inst_Server]
CopyFiles = atapi_copyfiles
AddReg = atapi_property_provider_AddReg

[atapi_Inst.Services]
AddService = atapi, %SPSVCINST_ASSOCSERVICE%, atapi_Service_Inst, atapi_EventLog_Inst

[atapi_Inst_Server.Services]
AddService = atapi, %SPSVCINST_ASSOCSERVICE%, atapi_Service_Inst_Server, atapi_EventLog_Inst

[atapi_Inst.HW]
AddReg = atapi_interrupt_priority_AddReg
AddReg = atapi_busdevicedesc_AddReg

[atapi_Inst_Server.HW]
AddReg = atapi_interrupt_priority_AddReg
AddReg = atapi_busdevicedesc_AddReg

[atapi_Inst.CoInstallers]
; empty section for compatibility

[atapi_Inst_Server.CoInstallers]
; empty section for compatibility

;*************************************************************
; atapi Service
[atapi_Service_Inst]
DisplayName    = %idechannel.DeviceDesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\atapi.sys
LoadOrderGroup = SCSI Miniport

[atapi_Service_Inst_Server]
DisplayName    = %idechannel.DeviceDesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\atapi.sys
LoadOrderGroup = SCSI Miniport
AddReg         = atapi_server_sku_values_AddReg

[atapi_EventLog_Inst]
AddReg = atapi_EventLog_AddReg

;*********************
; Add reg for atapi

[atapi_interrupt_priority_AddReg]
HKR,"Interrupt Management",,0x00000010
HKR,"Interrupt Management\Affinity Policy",,0x00000010
HKR,"Interrupt Management\Affinity Policy","DevicePriority",0x00010003,3

[atapi_property_provider_AddReg]
HKR,,EnumPropPages32,,"storprop.dll,AtaPropPageProvider"

[atapi_busdevicedesc_AddReg]
HKR,,UseBusDeviceDesc,%REG_DWORD%,1

[atapi_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_DWORD%,7

[atapi_server_sku_values_AddReg]
; Registry keys and values required for Server SKUs will be added in this section

;****************************************************
; Generic PCI IDE Controller 
[pciide_Inst]
CopyFiles = PciIde_CopyFiles, pciidex_copyfiles

[pciide_Inst.Services]
AddService = pciide, %SPSVCINST_ASSOCSERVICE%, pciide_Service_Inst

[pciide_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\pciide.sys
LoadOrderGroup = System Bus Extender

;**********************************************************
; Intel PCI IDE Controller 
[intelide_Inst]
CopyFiles = IntelIde_CopyFiles, pciidex_copyfiles
AddReg = intelChannelEnableCheck_AddReg.HW

[IntelIde_CopyFiles]
intelide.sys,,,0x100

[intelide_Inst.Services]
AddService = intelide, %SPSVCINST_ASSOCSERVICE%, intelide_Service_Inst

[intelide_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\intelide.sys
LoadOrderGroup = System Bus Extender

[intelChannelEnableCheck_AddReg.HW]
HKR,Channel0,ChannelStateMask,%REG_DWORD%,0x00000080
HKR,Channel0,ChannelStateOffset,%REG_DWORD%,0x00000041
HKR,Channel1,ChannelStateMask,%REG_DWORD%,0x00000080
HKR,Channel1,ChannelStateOffset,%REG_DWORD%,0x00000043

;**********************************************************
; SERVER WORKS PCI IDE Controller 
[serverworks_Inst]
CopyFiles = PciIde_CopyFiles, pciidex_copyfiles

[PciIde_CopyFiles]
pciide.sys,,,0x100

[serverworks_Inst.Services]
AddService = pciide, %SPSVCINST_ASSOCSERVICE%, pciide_Service_Inst

;****************************************************
; Generic AHCI Controller
; NOTE that the old section names [msahci_...] are used to install storahci.sys

[storahci_copyfiles]
storahci.sys,,,0x100

[msahci_Inst]
CopyFiles = storahci_copyfiles
AddPowerSetting=AhciPowerSetting1,AhciPowerSetting2

; Exclude Toshiba RAID controllers
ExcludeId = PCI\VEN_8086&DEV_2653&SUBSYS_0F001179
ExcludeId = PCI\VEN_8086&DEV_2653&SUBSYS_0F101179
ExcludeId = PCI\VEN_8086&DEV_27C5&SUBSYS_0F001179
ExcludeId = PCI\VEN_8086&DEV_27C5&SUBSYS_0F101179
ExcludeId = PCI\VEN_8086&DEV_27C5&SUBSYS_0F031179
ExcludeId = PCI\VEN_8086&DEV_27C5&SUBSYS_0F131179
ExcludeId = PCI\VEN_8086&DEV_27C5&SUBSYS_FF011179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_0F031179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_0F131179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF011179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF021179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF031179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF041179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF111179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF121179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF131179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF141179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF311179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF321179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF331179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF341179

[msahci_Inst_Server]
CopyFiles = storahci_copyfiles
AddPowerSetting=AhciPowerSetting1,AhciPowerSetting2

; Exclude Toshiba RAID controllers
ExcludeId = PCI\VEN_8086&DEV_2653&SUBSYS_0F001179
ExcludeId = PCI\VEN_8086&DEV_2653&SUBSYS_0F101179
ExcludeId = PCI\VEN_8086&DEV_27C5&SUBSYS_0F001179
ExcludeId = PCI\VEN_8086&DEV_27C5&SUBSYS_0F101179
ExcludeId = PCI\VEN_8086&DEV_27C5&SUBSYS_0F031179
ExcludeId = PCI\VEN_8086&DEV_27C5&SUBSYS_0F131179
ExcludeId = PCI\VEN_8086&DEV_27C5&SUBSYS_FF011179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_0F031179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_0F131179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF011179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF021179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF031179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF041179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF111179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF121179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF131179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF141179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF311179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF321179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF331179
ExcludeId = PCI\VEN_8086&DEV_2829&SUBSYS_FF341179

[AhciPowerSetting1]
Subgroup = {0012ee47-9041-4b5d-9b77-535fba8b1442}
; LPM: Partial - 10us resume time on IO; Slumber - 10ms resume time on IO

;****** HIPM settings 
Setting =  {0b2d69d7-a2a1-449c-9680-f91c70521c60}, "AHCI Link Power Management - HIPM/DIPM", "Configures the LPM state.",,0x00000001

Value = 0, "Active", "Neither Host or Device initiated allowed", 0x00010001, 0
Value = 1, "HIPM", "Host initiated allowed only", 0x00010001, 1
Value = 2, "HIPM+DIPM", "Both Host and Device initiated allowed", 0x00010001, 3 
Value = 3, "DIPM", "Device initiated allowed only", 0x00010001, 2

; High Performance
Default = {8C5E7FDA-E8BF-4A96-9A85-A6E23A8C635C}, 0, 0
Default = {8C5E7FDA-E8BF-4A96-9A85-A6E23A8C635C}, 1, 1
; Balanced
Default = {381B4222-F694-41F0-9685-FF5BB260DF2E}, 0, 1
Default = {381B4222-F694-41F0-9685-FF5BB260DF2E}, 1, 1
; Power Saving
Default = {A1841308-3541-4FAB-BC81-F71556F20B4A}, 0, 2
Default = {A1841308-3541-4FAB-BC81-F71556F20B4A}, 1, 2

[AhciPowerSetting2]
Subgroup = {0012ee47-9041-4b5d-9b77-535fba8b1442}
; LPM: Partial - 10us resume time on IO; Slumber - 10ms resume time on IO

;****** Partial to Slumber settings (ms)
Setting =  {DAB60367-53FE-4fbc-825E-521D069D2456}, "AHCI Link Power Management - Adaptive", "Automatically transit from Partial to Slumber.",,0x00000001
; range 0 to 5 minutes (unit: ms)
ValueRange = 0, 300000, 1, "millisecond"

; High Performance
Default = {8C5E7FDA-E8BF-4A96-9A85-A6E23A8C635C}, 0, 0
Default = {8C5E7FDA-E8BF-4A96-9A85-A6E23A8C635C}, 1, 0
; Balanced
Default = {381B4222-F694-41F0-9685-FF5BB260DF2E}, 0, 100
Default = {381B4222-F694-41F0-9685-FF5BB260DF2E}, 1, 100
; Power Saving
Default = {A1841308-3541-4FAB-BC81-F71556F20B4A}, 0, 100
Default = {A1841308-3541-4FAB-BC81-F71556F20B4A}, 1, 100

[msahci_Inst.HW]
AddReg=msahci_Inst_HW_AddReg

[msahci_Inst_Server.HW]
AddReg=msahci_Inst_HW_AddReg

[msahci_Inst_HW_AddReg]
; registry values related to MSI support
HKR, Interrupt Management, 0x00000010
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010
HKR, Interrupt Management\Affinity Policy, 0x00000010

;
; The MSISupported entry determines whether the device supports MSIs. Set it to 1 to enable MSI support.
;
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported,       %REG_DWORD%,   1

;
; The MessageNumberLimit entry specifies the maximum number of MSIs to allocate. 
; For PCI 2.2, MessageNumberLimit must be 1, 2, 4, 8, or 16. For PCI 3.0, MessageNumberLimit can be any number up to 2,048.
; Set it to 8 as it covers most of AHCI controller's needs that implement less than 8 ports.
;
HKR, Interrupt Management\MessageSignaledInterruptProperties, MessageNumberLimit, %REG_DWORD%,   8

;
; Make sure all processor in group are used to serve interrupt from this device. IrqPolicySpreadMessagesAcrossAllProcessors (5)
;
HKR, Interrupt Management\Affinity Policy, DevicePolicy,   %REG_DWORD%, 5

;
; Specifies that the device's interrupts are of high priority. This setting is appropriate for devices that require low latency. IrqPriorityHigh (3)
;
HKR, Interrupt Management\Affinity Policy, DevicePriority, %REG_DWORD%, 3

;
; Allow interrupt happens on processors beyond group 0. (e.g. might be in a single group other than 0)
;
HKR, Interrupt Management\Affinity Policy, GroupPolicy, %REG_DWORD%, 1

; Enables Storport IPM for this adapter
HKR, "StorPort", "EnableIdlePowerManagement", %REG_DWORD%, 0x01

[msahci_Inst.Services]
AddService = storahci, %SPSVCINST_ASSOCSERVICE%, msahci_Service_Inst_Client, storahci_EventLog_Inst

[msahci_Inst_Server.Services]
AddService = storahci, %SPSVCINST_ASSOCSERVICE%, msahci_Service_Inst_Server, storahci_EventLog_Inst

[msahci_Service_Inst_Client]
DisplayName    = %storahci_ServiceDescription%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\storahci.sys
LoadOrderGroup = SCSI Miniport
AddReg         = storahci_general_values
AddReg         = device_specific_values
AddReg         = client_sku_values
AddReg         = storahci_dmar_values

[msahci_Service_Inst_Server]
DisplayName    = %storahci_ServiceDescription%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_CRITICAL%
ServiceBinary  = %12%\storahci.sys
LoadOrderGroup = SCSI Miniport
AddReg         = storahci_general_values
AddReg         = device_specific_values
AddReg         = storahci_dmar_values

[storahci_general_values]
HKLM, "SYSTEM\CurrentControlSet\Control\Compatibility\Driver\storahci.sys", "Shims", %REG_MULTI_SZ_APPEND%, "Srbshim"

HKR, "Parameters\PnpInterface", "5", %REG_DWORD%, 0x00000001
HKR, "Parameters", "BusType", %REG_DWORD%, 0x0000000B
HKR, "Parameters", "IoTimeoutValue", %REG_DWORD%, 0x0000001E
HKR, "Parameters", "BusyRetryCount", %REG_DWORD%, 0x000000F0
HKR, "Parameters", "BusyPauseTimeInMs", %REG_DWORD%, 0x000001F4

[storahci_dmar_values]
; Default DMAR settings 2, where 2 = opt in, but only for external hot-plug devices
HKR, "Parameters", "DmaRemappingCompatible", %REG_DWORD%, 2

[device_specific_values]
HKR, "Parameters\Device", "ResetInInit", %REG_MULTI_SZ_APPEND%, "VEN_1106&DEV_6287&REV_*"

HKR, "Parameters\Device", "SingleIO", %REG_MULTI_SZ_APPEND%, "VEN_1106&DEV_6287&REV_00"
HKR, "Parameters\Device", "SingleIO", %REG_MULTI_SZ_APPEND%, "VEN_1106&DEV_6287&REV_10"
HKR, "Parameters\Device", "SingleIO", %REG_MULTI_SZ_APPEND%, "VEN_1106&DEV_6287&REV_20"

HKR, "Parameters\Device", "IgnoreHotPlug", %REG_MULTI_SZ_APPEND%, "VEN_1002&DEV_4380&REV_*"

HKR, "Parameters\Device", "NeverNonQueuedErrorRecovery", %REG_MULTI_SZ_APPEND%, "VEN_1002&DEV_4380&REV_*"

HKR, "Parameters\Device", "EnableCLOReset", %REG_MULTI_SZ_APPEND%, "VEN_1002&DEV_4391&REV_*"

HKR, "Parameters\Device", "ExpectedMsiMessageCount", %REG_MULTI_SZ_APPEND%, "VEN_1022&DEV_7801&REV_00 8"

HKR, "Parameters\Device", "NoFUACommand", %REG_MULTI_SZ_APPEND%, "HTE*"
HKR, "Parameters\Device", "NoFUACommand", %REG_MULTI_SZ_APPEND%, "Hitachi*"
HKR, "Parameters\Device", "NoFUACommand", %REG_MULTI_SZ_APPEND%, "HTS*"
HKR, "Parameters\Device", "NoFUACommand", %REG_MULTI_SZ_APPEND%, "HDS*"
HKR, "Parameters\Device", "NoFUACommand", %REG_MULTI_SZ_APPEND%, "HDT*"

HKR, "Parameters\Device", "NeedSetTransferModeCommand", %REG_MULTI_SZ_APPEND%, "MCBQE64GBMPP*"

HKR, "Parameters\Device", "NoLPM", %REG_MULTI_SZ_APPEND%, "WD740ADFD?00NLR1*"
HKR, "Parameters\Device", "NoLPM", %REG_MULTI_SZ_APPEND%, "WDC WD740ADFD?00NLR1*"
HKR, "Parameters\Device", "NoLPM", %REG_MULTI_SZ_APPEND%, "Maxtor 6V???E0*"
HKR, "Parameters\Device", "NoLPM", %REG_MULTI_SZ_APPEND%, "Maxtor 6V???F0*"
HKR, "Parameters\Device", "NoLPM", %REG_MULTI_SZ_APPEND%, "Maxtor 7V???E0*"
HKR, "Parameters\Device", "NoLPM", %REG_MULTI_SZ_APPEND%, "Maxtor 7V???F0*"
HKR, "Parameters\Device", "NoLPM", %REG_MULTI_SZ_APPEND%, "SanDisk SSD P4*"

HKR, "Parameters\Device", "NoIdleD3", %REG_MULTI_SZ_APPEND%, "INTEL SSD?C??????A4"
HKR, "Parameters\Device", "NoIdleD3", %REG_MULTI_SZ_APPEND%, "INTEL SSD?C??????A4?"
HKR, "Parameters\Device", "NoIdleD3", %REG_MULTI_SZ_APPEND%, "INTEL SSD?C??????A4??"
HKR, "Parameters\Device", "NoIdleD3", %REG_MULTI_SZ_APPEND%, "INTEL SSD?C??????A5"
HKR, "Parameters\Device", "NoIdleD3", %REG_MULTI_SZ_APPEND%, "INTEL SSD?C??????A5?"
HKR, "Parameters\Device", "NoIdleD3", %REG_MULTI_SZ_APPEND%, "INTEL SSD?C??????A5??"

HKR, "Parameters\Device", "PRDTSplit", %REG_MULTI_SZ_APPEND%, "VEN_1022&DEV_43B5&REV_*"
HKR, "Parameters\Device", "PRDTSplit", %REG_MULTI_SZ_APPEND%, "VEN_1022&DEV_43B6&REV_*"
HKR, "Parameters\Device", "PRDTSplit", %REG_MULTI_SZ_APPEND%, "VEN_1022&DEV_43B7&REV_*"
HKR, "Parameters\Device", "PRDTSplit", %REG_MULTI_SZ_APPEND%, "VEN_1022&DEV_43B8&REV_*"
HKR, "Parameters\Device", "PRDTSplit", %REG_MULTI_SZ_APPEND%, "VEN_1022&DEV_43C8&REV_*"

; this part is specific for Client SKUs
[client_sku_values]
HKR, "Parameters", "IoLatencyCap", %REG_DWORD%, 0x000001F4

[storahci_EventLog_Inst]
AddReg = storahci_EventLog_AddReg

[storahci_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_DWORD%,7

;********************************************************
; Extra Registry Entries

[Strings]
;Localizable
MS                      = "Microsoft"
MS-Drivers              = "(Standard IDE ATA/ATAPI controllers)"
idechannel.DeviceDesc   = "IDE Channel"
PCI\CC_0101.DeviceDesc  = "Standard Dual Channel PCI IDE Controller"
SERVERWORKS="ServerWorks"
PCI\VEN_1166&DEV_0211.DeviceDesc="OSB4 IDE Controller"
PCI\VEN_1166&DEV_0212&SUBSYS_02121166.DeviceDesc="CSB5 IDE Controller"
INTEL="Intel"
PCI\VEN_8086&DEV_1222.DeviceDesc="Intel(R) 82092AA PCI IDE Controller"
PCI\VEN_8086&DEV_1230.DeviceDesc="Intel(R) 82371FB PCI Bus Master IDE Controller"
PCI\VEN_8086&DEV_7010.DeviceDesc="Intel(R) 82371SB PCI Bus Master IDE Controller"
PCI\VEN_8086&DEV_7111.DeviceDesc="Intel(R) 82371AB/EB PCI Bus Master IDE Controller"
PCI\VEN_8086&DEV_2411.DeviceDesc="Intel(R) 82801AA Bus Master IDE Controller"
PCI\VEN_8086&DEV_2421.DeviceDesc="Intel(R) 82801AB Bus Master IDE Controller"
PCI\VEN_8086&DEV_7199.DeviceDesc="Intel(R) 82440MX Bus Master IDE Controller"
PCI\VEN_8086&DEV_244A.DeviceDesc="Intel(R) 82801BAM Ultra ATA Storage Controller - 244A"
PCI\VEN_8086&DEV_244B.DeviceDesc="Intel(R) 82801BA Ultra ATA Storage Controller - 244B"
PCI\VEN_8086&DEV_248A.DeviceDesc="Intel(R) 82801CAM Ultra ATA Storage Controller-248A"
PCI\VEN_8086&DEV_248B.DeviceDesc="Intel(R) 82801CA Ultra ATA Storage Controller-248B"
PCI\VEN_8086&DEV_24C1.DeviceDesc="Intel(R) 82801DBM Ultra ATA Storage Controller - 24C1"
PCI\VEN_8086&DEV_24CA.DeviceDesc="Intel(R) 82801DBM Ultra ATA Storage Controller - 24CA"
PCI\VEN_8086&DEV_24CB.DeviceDesc="Intel(R) 82801DB Ultra ATA Storage Controller-24CB"
PCI\VEN_8086&DEV_24D1.DeviceDesc="Intel(R) 82801EB Ultra ATA Storage Controllers - 24D1"
PCI\VEN_8086&DEV_24DB.DeviceDesc="Intel(R) 82801EB Ultra ATA Storage Controllers - 24DB"
PCI\VEN_8086&DEV_25A2.DeviceDesc="Intel(R) 6300ESB Ultra ATA Storage Controller - 25A2"
PCI\VEN_8086&DEV_25A3.DeviceDesc="Intel(R) 6300ESB Ultra ATA Storage/SATA Controller - 25A3" 
PCI\VEN_8086&DEV_2651.DeviceDesc="Intel(R) 82801FB Ultra ATA Storage Controllers - 2651"
PCI\VEN_8086&DEV_2652.DeviceDesc="Intel(R) 82801FB Ultra ATA Storage Controllers - 2652"
PCI\VEN_8086&DEV_2653.DeviceDesc="Intel(R) 82801FBM Ultra ATA Storage Controllers - 2653"
PCI\VEN_8086&DEV_266F.DeviceDesc="Intel(R) 82801FB/FBM Ultra ATA Storage Controllers - 266F"
PCI\VEN_8086&DEV_7601.DeviceDesc="Intel(R) IA64 Bus Master IDE Controller"
PCI\VEN_8086&DEV_27C0.DeviceDesc="Intel(R) 82801GB/GR/GH (ICH7 Family) Serial ATA Storage Controller - 27C0"
PCI\VEN_8086&DEV_27C4.DeviceDesc="Intel(R) 82801GBM/GHM (ICH7-M Family) Serial ATA Storage Controller - 27C4"
PCI\VEN_8086&DEV_27DF.DeviceDesc="Intel(R) 82801G (ICH7 Family) Ultra ATA Storage Controllers - 27DF"
PCI\VEN_8086&DEV_2820.DeviceDesc="Intel(R) ICH8 4 port Serial ATA Storage Controller - 2820"
PCI\VEN_8086&DEV_2825.DeviceDesc="Intel(R) ICH8 2 port Serial ATA Storage Controller - 2825"
PCI\VEN_8086&DEV_2828.DeviceDesc="Intel(R) ICH8M 3 port Serial ATA Storage Controller - 2828"
PCI\VEN_8086&DEV_2850.DeviceDesc="Intel(R) ICH8M Ultra ATA Storage Controllers - 2850"

SIS="Silicon Integrated System"
PCI\VEN_1039&DEV_0601.DeviceDesc="SiS PCI IDE Controller"
PCI\VEN_1039&DEV_5513.DeviceDesc="SiS PCI IDE Controller"

IBM="IBM"
PCMCIA\IBM-MICRODRIVE-7F50.DeviceDesc="IBM Microdrive"
PCMCIA\IBM-MICRODRIVE-AA55.DeviceDesc="IBM Microdrive"
SONY="SONY"
PCMCIA\SONY-MEMORYSTICK.DeviceDesc="Sony Memory Stick" 
LEXAR="Lexar Microsystems"
LEXAR.DeviceDesc="Lexar Media Digital Film Card"
NVIDIA="NVIDIA"
PCI\VEN_10DE&DEV_00E3.DeviceDesc="NVIDIA nForce3 250 Serial ATA Controller"
PCI\VEN_10DE&DEV_00E5.DeviceDesc="NVIDIA nForce3 250 Parallel ATA Controller"
PCI\VEN_10DE&DEV_00EE.DeviceDesc="NVIDIA nForce3 250 Serial ATA Controller"

pcmcia.DeviceDesc               = "PCMCIA IDE/ATAPI Controller"

storahci_ServiceDescription = "Microsoft Standard SATA AHCI Driver"
MS-AHCI="Standard SATA AHCI Controller"
PCI\CC_010601.DeviceDesc  = "Standard SATA AHCI Controller"
ACPI\CLS_0001&SUBCLS_0006&PI_01.DeviceDesc = "Standard SATA AHCI Controller"
ACPI\AMDI0600.DeviceDesc = "<TEMP> AMD SoC SATA AHCI Controller"

;*******************************************
;Non-localizable, Handy macro substitutions
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
SERVICE_ERROR_CRITICAL = 3
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
REG_MULTI_SZ           = 0x00010000
REG_MULTI_SZ_APPEND    = 0x00010008
